(footprint "HDMI_A_Molex_208658-1001_Horizontal"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "HDMI Molex Type A https://www.molex.com/pdm_docs/sd/2086581001_sd.pdf")
	(tags "HDMI Molex Type A")
	(property "Reference" "REF**"
		(at -5.26 -7.8 90)
		(layer "F.SilkS")
		(uuid "89d5d15f-b722-43a1-a497-6cf360b42655")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "HDMI_A"
		(at 1.715 10 0)
		(layer "F.Fab")
		(uuid "d6cbb287-a312-44a7-a5d5-a0c51a223951")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_HDMI:HDMI_A_Molex_208658-1001_Horizontal"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e8a18617-5864-432c-827e-4866c62bc178")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" "https://en.wikipedia.org/wiki/HDMI"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fc9d8a38-1956-4f78-8fcb-42259eff3ebb")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "125d7647-b8e9-4bb3-ba82-81923d37d230")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "d30bd262-cc1d-4f48-9bec-a28ab72222bb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "直插式HDMI母座-19Pin(19PIN)"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "7478eb2f-fad2-4e32-8a46-85560afca93c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "e933bb18-14d5-4d9b-969f-ecb9ed3194a2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ff8b1380-2a6a-4d32-85e0-1c2a009d5211")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -4.985 -4.9)
		(end -4.235 -4.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8b193746-10d5-4d58-a95e-701f99288b61")
	)
	(fp_line
		(start -4.235 -4.9)
		(end -4.235 -6.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3644f40e-4548-4e5c-9170-3e0206046f1b")
	)
	(fp_line
		(start -4.235 6.7)
		(end -4.235 4.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "35d62f57-ccc8-42da-845b-89a57421cd5c")
	)
	(fp_line
		(start -0.685 -7.61)
		(end 2.115 -7.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f05f3b10-e432-429e-ab53-1ab048642c3e")
	)
	(fp_line
		(start -0.685 7.61)
		(end 2.115 7.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3c41b9e1-fde2-428d-9556-218b9aa74a0a")
	)
	(fp_line
		(start 4.815 -7.61)
		(end 6.915 -7.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0f072e77-7a29-41cc-9c54-d97c0b409a50")
	)
	(fp_line
		(start 4.815 7.61)
		(end 6.915 7.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2037eda7-c5db-42d2-82d9-9d8cd6a115d1")
	)
	(fp_line
		(start 7.025 -7.5)
		(end 7.025 7.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "b5086cab-4aed-4571-ab75-a716684bebf0")
	)
	(fp_line
		(start -5.09 5.15)
		(end -5.09 -5.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "21decb72-91a1-4875-9fdd-ab2aa39da7d2")
	)
	(fp_line
		(start -4.69 -5.15)
		(end -5.09 -5.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5be644ae-b759-444b-8d1c-379200f2e362")
	)
	(fp_line
		(start -4.69 -5.15)
		(end -4.69 -8.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "36abd382-178a-4274-9699-770df4d30e51")
	)
	(fp_line
		(start -4.69 5.15)
		(end -5.09 5.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b86b398c-aab4-430c-942d-1e4def743231")
	)
	(fp_line
		(start -4.69 8.5)
		(end -4.69 5.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6c0ac8a4-8908-463b-a212-8dda21d8c313")
	)
	(fp_line
		(start -0.96 -8.5)
		(end -4.69 -8.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a9124089-418e-4ca6-b558-cfbe530175f7")
	)
	(fp_line
		(start -0.96 -8.1)
		(end -0.96 -8.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4bc43103-d01e-4f3c-bebf-290a279e55de")
	)
	(fp_line
		(start -0.96 8.5)
		(end -4.69 8.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2056d17c-6800-4b04-9e80-a4c6c33be44c")
	)
	(fp_line
		(start -0.96 8.5)
		(end -0.96 8.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a12cee22-48c8-4b67-b813-724887784d47")
	)
	(fp_line
		(start 2.37 -8.1)
		(end -0.96 -8.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2fa93c37-a178-4dd9-b47d-630dfccc54f6")
	)
	(fp_line
		(start 2.37 -8.1)
		(end 2.37 -8.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ad3b51f5-247f-44e6-a8e8-d2d673626ac3")
	)
	(fp_line
		(start 2.37 8.1)
		(end -0.96 8.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "772e3340-bcf6-4c81-adbd-446908fbed7c")
	)
	(fp_line
		(start 2.37 8.5)
		(end 2.37 8.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5eec31d8-eec5-46fb-85b8-1a8f27eafc95")
	)
	(fp_line
		(start 4.52 -8.5)
		(end 2.37 -8.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a71c734c-31d4-4deb-8212-2727387ac841")
	)
	(fp_line
		(start 4.52 -8.1)
		(end 4.52 -8.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "17faa409-daf5-4143-9ba4-e5752c767703")
	)
	(fp_line
		(start 4.52 8.5)
		(end 2.37 8.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "40ce8ba7-02ec-4717-a1a3-7bb25273cd99")
	)
	(fp_line
		(start 4.52 8.5)
		(end 4.52 8.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2fadbed8-cebf-4791-b3fc-536f80be9b9b")
	)
	(fp_line
		(start 8.53 -8.1)
		(end 4.52 -8.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d5f76f74-e0b0-4402-9cb8-655d604162ac")
	)
	(fp_line
		(start 8.53 8.1)
		(end 4.52 8.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "00b15d2f-25fe-45f9-a5a6-ebe22a75b9a9")
	)
	(fp_line
		(start 8.53 8.1)
		(end 8.53 -8.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "abb52fc7-dc6e-42d7-9004-d19fe5d64fef")
	)
	(fp_line
		(start -4.125 -7.5)
		(end -4.125 7.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9c3e343a-472c-46c1-a6f4-5bd016fb7872")
	)
	(fp_line
		(start -4.125 -7.5)
		(end 8.025 -7.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d24be083-e220-46e6-880c-3f887acf0a99")
	)
	(fp_line
		(start -4.125 7.5)
		(end 8.025 7.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "02181782-cf25-4896-866f-7a2c9333b4e3")
	)
	(fp_line
		(start 8.025 -7.5)
		(end 8.025 7.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9229a419-7e3a-4777-8d59-352d204febff")
	)
	(fp_text user "PCB Edge"
		(at 5.715 0 90)
		(layer "Dwgs.User")
		(uuid "9954fced-96ee-4225-beec-ca9701dfd390")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 1.715 0 0)
		(layer "F.Fab")
		(uuid "cc1df25c-5820-4b8d-8199-9c0f352ed75f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -3.285 -4.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "251edfdf-10b4-4f16-ba71-644c324321ac")
	)
	(pad "2" smd rect
		(at -3.285 -4)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "63a501c6-cae2-4cf1-8f02-ee739e12b49b")
	)
	(pad "3" smd rect
		(at -3.285 -3.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "b51a002a-cd25-4545-9305-7bc4050f51b9")
	)
	(pad "4" smd rect
		(at -3.285 -3)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c0f12344-324e-4e9f-bbc2-a9546c7c6d45")
	)
	(pad "5" smd rect
		(at -3.285 -2.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "696e0084-8a8c-4367-91b1-408cbbe53881")
	)
	(pad "6" smd rect
		(at -3.285 -2)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "d9af5282-971f-42d0-8b92-f057d06d9528")
	)
	(pad "7" smd rect
		(at -3.285 -1.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "bd27f3aa-308d-43f6-ac33-ccde0afa6f0b")
	)
	(pad "8" smd rect
		(at -3.285 -1)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "d6a020ef-32d1-4874-ac10-bd23edaea34c")
	)
	(pad "9" smd rect
		(at -3.285 -0.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "0c3df432-3a16-4b31-aac1-8ca68670a534")
	)
	(pad "10" smd rect
		(at -3.285 0)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "deed6e36-d1a5-4b7f-b2c8-259bcdb788af")
	)
	(pad "11" smd rect
		(at -3.285 0.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "70748c05-f1f1-4ad1-8ed7-1a3c872b49ed")
	)
	(pad "12" smd rect
		(at -3.285 1)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "5bf657b8-0d92-4700-ac7a-aa3477d60d13")
	)
	(pad "13" smd rect
		(at -3.285 1.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "d8d7f161-6fef-4234-89b0-967f1ad8473b")
	)
	(pad "14" smd rect
		(at -3.285 2)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "574bd2e8-46da-414a-b3e1-d9319b40074a")
	)
	(pad "15" smd rect
		(at -3.285 2.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "a3e05f2f-03d4-4c20-a6b5-639d34446da3")
	)
	(pad "16" smd rect
		(at -3.285 3)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "8b564b9a-107e-4ce2-9cff-1b7263d6f8af")
	)
	(pad "17" smd rect
		(at -3.285 3.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "491814ba-81a2-4db1-95e6-d2dcd6423700")
	)
	(pad "18" smd rect
		(at -3.285 4)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "799d767e-076d-4dd9-b02d-91d614ae47cf")
	)
	(pad "19" smd rect
		(at -3.285 4.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "9ed640dd-09d1-43d2-a43f-4b8b5fa898d4")
	)
	(pad "SH" thru_hole oval
		(at -2.525 -7.25)
		(size 3.3 1.5)
		(drill oval 2.7 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "92641b80-a7b7-4f84-bc8b-c8f1e5612dcd")
	)
	(pad "SH" thru_hole oval
		(at -2.525 7.25)
		(size 3.3 1.5)
		(drill oval 2.7 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "025e1992-507f-47fd-b777-cf78dab2e990")
	)
	(pad "SH" thru_hole oval
		(at 3.435 -7.25)
		(size 2.3 1.5)
		(drill oval 1.7 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "7f981b49-3867-4896-867e-ffae9eab51e7")
	)
	(pad "SH" thru_hole oval
		(at 3.435 7.25)
		(size 2.3 1.5)
		(drill oval 1.7 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "307b43c1-6a38-4d0c-9215-9ff3aedf95d0")
	)
	(model "${KICAD6_3DMODEL_DIR}/Connector_HDMI.3dshapes/HDMI_A_Molex_208658-1001_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)