(footprint "LED_0603_1608Metric"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
	(tags "LED")
	(property "Reference" "REF**"
		(at 0 -1.43 0)
		(layer "F.SilkS")
		(uuid "292741c4-f38a-46be-96b4-e8e4adda1eb8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "LED_0603_1608Metric"
		(at 0 1.43 0)
		(layer "F.Fab")
		(uuid "53d18d0d-7a8b-4ada-90ab-6382184ad4c2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "caff2e29-3491-4ab9-a3eb-0ab70a5ce5f4")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3dcc49b9-49cf-44c1-805a-80a6e05abd5a")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e40f0117-981e-4235-9a99-7538c3a8ca9e")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.485 -0.735)
		(end -1.485 0.735)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a61009e0-7d1c-4008-bc11-4b210fbb5f45")
	)
	(fp_line
		(start -1.485 0.735)
		(end 0.8 0.735)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "14a2ba1c-1389-4245-b264-01e350a58427")
	)
	(fp_line
		(start -0.29 0.02)
		(end 0.21 -0.33)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ec97b614-96d8-4bcd-bed7-3480b9b601bd")
	)
	(fp_line
		(start 0.21 -0.33)
		(end 0.21 0.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "821c2eed-be46-4708-9589-4176811bc6d3")
	)
	(fp_line
		(start 0.21 0.37)
		(end -0.29 0.02)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c6d677af-229a-48f6-839a-089216337b12")
	)
	(fp_line
		(start 0.8 -0.735)
		(end -1.485 -0.735)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ca086f38-23cb-437f-98b5-9eb3543ea14c")
	)
	(fp_line
		(start -1.48 -0.73)
		(end 1.48 -0.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5f061956-b91d-45f4-b57f-38aeb40795c3")
	)
	(fp_line
		(start -1.48 0.73)
		(end -1.48 -0.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2dde7546-5f04-46b7-ad48-8cf9f8394899")
	)
	(fp_line
		(start 1.48 -0.73)
		(end 1.48 0.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7bfde076-eefc-4f5b-8e45-4f5e4bf15a48")
	)
	(fp_line
		(start 1.48 0.73)
		(end -1.48 0.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "86486440-4856-4c98-ad7d-3958c0cdb18d")
	)
	(fp_line
		(start -0.8 -0.1)
		(end -0.8 0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "98c2e268-ea04-482a-83b8-8f38c3203b78")
	)
	(fp_line
		(start -0.8 0.4)
		(end 0.8 0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "af641bc8-d996-4a2a-895a-06d3b5ad3322")
	)
	(fp_line
		(start -0.5 -0.4)
		(end -0.8 -0.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "087d096f-0c5a-4d2c-ad5f-1bef65ca374d")
	)
	(fp_line
		(start 0.8 -0.4)
		(end -0.5 -0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e85c8247-c2d8-4e42-8fe5-79ef729f3ed5")
	)
	(fp_line
		(start 0.8 0.4)
		(end 0.8 -0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "496d1695-30f2-45b1-a793-58b2f6fdd52b")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "1d693d84-fdc3-48eb-afa5-40e190cdca80")
		(effects
			(font
				(size 0.4 0.4)
				(thickness 0.06)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.7875 0)
		(size 0.875 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "902f25b0-cb45-4114-bb5f-def34f8704c7")
	)
	(pad "2" smd roundrect
		(at 0.7875 0)
		(size 0.875 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "dd9eecb5-87cb-42a6-baae-af0c098b27ff")
	)
	(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)