(footprint "DC_Jack_DC007B_30V_10A"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 2.99 13.905 180)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "4e1c214c-388c-4cf9-b7f9-82fee53d671a")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Barrel_Jack_Switch"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "685755d1-8ec3-4c5e-ba62-4bc86ccc7d7d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Library:DC_Jack_DC007B_30V_10A"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c65a00bb-1a1b-427e-a0c1-37821a3d6c95")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "16976c29-2b7e-45b8-866f-854d636184b9")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a6452ee7-40bb-4764-8374-256c47e419f4")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" "https://item.szlcsc.com/19360929.html"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "119c9f9f-41d6-42c9-835d-4e197b9cab09")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "12V/10A DC2.5母座"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "cc81d113-e9af-47b4-a0db-39f4d11e1e22")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "9b2dba93-eaa4-457d-9277-9925a4de7b39")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ba370566-174b-4105-b30c-6c9fc320b5cf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start 5 0)
		(end -5 13)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "71028170-b2f7-4871-b2e8-eca9496a58e3")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "6c5e7548-d3da-4511-a88b-e4163f7b936c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 2.75)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "F&B.Cu" "*.Mask")
		(uuid "b5b40111-c929-4c35-b5d7-2ac336aecd36")
	)
	(pad "1" thru_hole circle
		(at 0 12)
		(size 2.2 2.2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "83c3f5ca-e1e1-4ba5-92d5-3dc5d8f595be")
	)
	(pad "2" thru_hole oval
		(at 0 6 90)
		(size 1.5 3.7)
		(drill oval 0.8 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "95602671-8e16-466b-99c9-871b1ab18b82")
	)
	(pad "3" thru_hole oval
		(at -4.75 5.5)
		(size 1.5 2.7)
		(drill oval 0.8 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "5f8a57a1-cf5d-4df6-a41c-1199eb43aba7")
	)
	(pad "3" thru_hole oval
		(at -4.75 10.2)
		(size 1.5 2.7)
		(drill oval 0.8 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "a31f1789-f680-4829-979c-2b2915f5d067")
	)
	(pad "3" thru_hole oval
		(at 4.75 5.5)
		(size 1.5 2.7)
		(drill oval 0.8 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "367dc31c-c8da-4071-82af-313ca0280efa")
	)
	(pad "3" thru_hole oval
		(at 4.75 10.1)
		(size 1.5 2.7)
		(drill oval 0.8 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "b85166d9-4371-429f-a7f0-779ea3e0a1b5")
	)
	(model "D:/download_LCEDA_3D_Model/DC-IN-TH_HX-DC007B-2.009.step"
		(offset
			(xyz 0 -6.5 5.1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)