(footprint "C_0603_1608Metric"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "capacitor")
	(property "Reference" "REF**"
		(at 2.35 -0.02 180)
		(layer "F.SilkS")
		(uuid "be18dbb0-59da-41ff-a9b6-0d40e490650c")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "22uF/10V"
		(at 0 1.43 180)
		(layer "F.Fab")
		(uuid "e2ef7e5c-08ba-4883-82ff-f40cff5df973")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2d12633d-f05b-48f9-b7a2-fffaaf87966a")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f7cdb2ae-503f-4d07-a17b-261230aad32d")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e47eb9cd-e47d-4f0d-b97a-c5f8cf37c4d1")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "06faf791-596a-4c75-9177-bd32a5fdb558")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "贴片电容0603-22uF-10V-X5R(0603)"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "63a43ead-8963-4e6c-a0d1-ba735107bac0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" "C603"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "e1f22653-f9bf-4c2e-ad4c-6ce49787d488")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8273c90c-960d-4afd-a7e2-d3844e3b3146")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.14058 -0.51)
		(end 0.14058 -0.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8b13d5e8-366e-48bb-a8de-a5f7b1659c0a")
	)
	(fp_line
		(start -0.14058 0.51)
		(end 0.14058 0.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1abe67a2-1039-4488-a401-2a49ae870914")
	)
	(fp_line
		(start -1.48 -0.73)
		(end 1.48 -0.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "bca0c0b7-68d8-4378-a1c8-5cd60bd0d008")
	)
	(fp_line
		(start -1.48 0.73)
		(end -1.48 -0.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8008b46c-2036-457c-91fc-a1e3f162ba1d")
	)
	(fp_line
		(start 1.48 -0.73)
		(end 1.48 0.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "35e7ae85-30af-422d-80ac-692c9b30cf51")
	)
	(fp_line
		(start 1.48 0.73)
		(end -1.48 0.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7564bb10-5ea2-4a60-8094-10c81b8d5371")
	)
	(fp_line
		(start -0.8 -0.4)
		(end 0.8 -0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "20af8c02-bad8-4291-b397-8656d1499e8f")
	)
	(fp_line
		(start -0.8 0.4)
		(end -0.8 -0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ea453e1f-3a0a-4c5f-9a2d-3ad645d0bc70")
	)
	(fp_line
		(start 0.8 -0.4)
		(end 0.8 0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9c4f0471-8bd8-4aea-a76b-a07a74d6b880")
	)
	(fp_line
		(start 0.8 0.4)
		(end -0.8 0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "36ed09d3-e1fb-45ca-b2fc-3c69be4c4f28")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "74fdb512-a26e-41cb-b5a4-d455f6b1b244")
		(effects
			(font
				(size 0.4 0.4)
				(thickness 0.06)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.775 0)
		(size 0.9 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "fd8de1f0-b987-4a87-b356-2ab49e55616a")
	)
	(pad "2" smd roundrect
		(at 0.775 0)
		(size 0.9 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "e262509f-b90d-42cf-a6b6-01d4c662ac91")
	)
	(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)