(footprint "PinHeader_1x03_P2.54mm_Vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
	(tags "Through hole pin header THT 1x03 2.54mm single row")
	(property "Reference" "REF**"
		(at -0.11 7.6 -90)
		(layer "F.SilkS")
		(hide yes)
		(uuid "84fa010e-5aae-408b-88bc-9c3f11d8958b")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Conn_01x03_Pin"
		(at 0 7.41 0)
		(layer "F.Fab")
		(uuid "e7d55716-bc0a-40a9-a805-ba44f2ac7f51")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6fbbb2e2-8cf7-4386-bc8b-39c67cd618c8")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9d16db71-20ea-4da1-80b0-5c8a657a19c2")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2efb4633-c851-41fe-8e75-d091833e10b5")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "DF_Comment" "2.54红色单排排针-3P"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "a417d529-cdd1-48c1-8e64-8213bcdd7149")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7ee4100f-d6b7-421e-9cbb-d4c6f20c5d7a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.33 -1.33)
		(end 0 -1.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3df1f677-045b-4aae-9fcf-eb042cfadeda")
	)
	(fp_line
		(start -1.33 0)
		(end -1.33 -1.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dfb25e45-4bfc-4687-94ac-3ace491c1048")
	)
	(fp_line
		(start -1.33 1.27)
		(end -1.33 6.41)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4bf5b0b3-f9cc-4024-b33e-12f4008ad195")
	)
	(fp_line
		(start -1.33 1.27)
		(end 1.33 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "40e6eec0-f267-452e-a3cd-32315e71101d")
	)
	(fp_line
		(start -1.33 6.41)
		(end 1.33 6.41)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6bf7b614-1e96-4e95-bd6d-c266f4656c34")
	)
	(fp_line
		(start 1.33 1.27)
		(end 1.33 6.41)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "81f72081-a04e-4585-ade3-7ec0d54fff87")
	)
	(fp_line
		(start -1.8 -1.8)
		(end -1.8 6.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e82e7743-effd-4304-ace2-1c2b36a62d44")
	)
	(fp_line
		(start -1.8 6.85)
		(end 1.8 6.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9e2e0856-47ef-490e-b633-d68d21e17c81")
	)
	(fp_line
		(start 1.8 -1.8)
		(end -1.8 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b7f733f7-ba4f-45c0-886d-31334198707f")
	)
	(fp_line
		(start 1.8 6.85)
		(end 1.8 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d9c3b7fd-5de1-4198-9038-10fd534cb54b")
	)
	(fp_line
		(start -1.27 -0.635)
		(end -0.635 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "116e3d60-7140-46ef-8cf0-adc80baa9644")
	)
	(fp_line
		(start -1.27 6.35)
		(end -1.27 -0.635)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "187f5ae1-386b-459d-bf98-bd32d47cf6b4")
	)
	(fp_line
		(start -0.635 -1.27)
		(end 1.27 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7fd59471-6394-44d5-92e8-875f61cec8dc")
	)
	(fp_line
		(start 1.27 -1.27)
		(end 1.27 6.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f76866f4-3863-4a49-a26d-c3433f64bf39")
	)
	(fp_line
		(start 1.27 6.35)
		(end -1.27 6.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a55b8ed5-5137-4254-ad0a-8c1c56ee73b9")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.54 90)
		(layer "F.Fab")
		(uuid "265f2fe7-8ccd-4a93-b71c-e4d851a69cc0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c08b3d9f-664e-4c4f-b75e-3b974dac8c02")
	)
	(pad "2" thru_hole oval
		(at 0 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c44304a9-a933-4da5-b761-1c69eb451316")
	)
	(pad "3" thru_hole oval
		(at 0 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "643dd865-4d5b-47e5-9d72-233b9666575f")
	)
	(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)