(footprint "MountingHole_3mm_M2_Pad_TopOnly"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3e212f2a-eff9-4b8f-9a96-3e5e3a53a53f")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "MountingHole_3mm_M2_Pad_TopOnly"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "97db3b4a-82fb-42bb-a83f-66403bd025da")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0b1fb5f8-515f-4cf7-a4ff-d6007aa61146")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6988df79-8749-4079-8912-157387ac1577")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "01455100-f4fc-4b51-bd61-f181dee2d5fd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_circle
		(center 0 0)
		(end 2.8 0)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill none)
		(layer "Cmts.User")
		(uuid "028c0e88-f008-4a61-966a-8f5a06c6f991")
	)
	(fp_circle
		(center 0 0)
		(end 3.05 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "45203c13-6cc6-4c86-8ffd-f5c4e2fe30cb")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "7ce8978f-93a0-4078-ae78-b92fbef48f6f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3.2 3.2)
		(drill 3.05)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "09371e93-6a2a-4022-ad14-586e90ca1785")
	)
	(pad "1" connect circle
		(at 0 0)
		(size 4.4 4.4)
		(layers "F.Cu" "F.Mask")
		(uuid "f78969f4-3f06-4471-9820-636e07f3f0c5")
	)
)