(footprint "SW_Push_6x6x6"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "1ad0f44b-ce26-46b8-8bd0-ce5c45516250")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "SW_Push_6x6x6"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "7e0a81f4-2a8a-431b-bb3e-14de0894c973")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "02c1ac68-b351-4ec2-aabd-e4991765fa5e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1afff2d4-80c8-43f2-932e-2c1760e57f9f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "53a5a7ff-5cfa-40f5-8a84-4370c60a2354")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -3 -3)
		(end 3 3)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "c34633d0-ff13-461c-89fb-608c9b220e68")
	)
	(fp_circle
		(center -2 -2)
		(end -1.5 -2)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "45c65389-e882-46f0-a599-8ba3e4910dd4")
	)
	(fp_circle
		(center -2 2)
		(end -2 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "d5448b2e-29d6-40df-a154-531335a73514")
	)
	(fp_circle
		(center 0 0)
		(end 1.75 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "9797c0e8-3955-4553-8627-19da6b8ed211")
	)
	(fp_circle
		(center 2 -2)
		(end 2.5 -2)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "0299c211-d64f-442f-8919-058a93a283d9")
	)
	(fp_circle
		(center 2 2)
		(end 2.5 2)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "ac454912-b0d7-46ec-b25f-e74bb4dfd698")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "e8835f99-db0a-4bfe-86be-f468039428fa")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -4 -2.25)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "ec6d8abd-ec9c-4087-9c5b-29269731b0ea")
	)
	(pad "1" smd roundrect
		(at 4 -2.25)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "9ceb137a-b387-4e69-949f-eb2abb38060b")
	)
	(pad "2" smd roundrect
		(at -4 2.25)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "61607888-d9a1-40e5-8c9c-0e6ba6bb3c54")
	)
	(pad "2" smd roundrect
		(at 4 2.25)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "5064e1d3-81ef-4393-94e4-6f9765c029f3")
	)
	(model "G:/download_LCEDA_3D_Model/KEY-SMD_4P-L6.0-W6.0-H5.0-LS10.0-P4.053.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)