(footprint "PinHeader_1x04_P2.54mm_Vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
	(tags "Through hole pin header THT 1x04 2.54mm single row")
	(property "Reference" "REF**"
		(at 0 -2.52 90)
		(layer "F.SilkS")
		(hide yes)
		(uuid "02b1d5de-a4aa-486e-817a-3173ba37c9cd")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Conn_01x04_Pin"
		(at 0 9.95 180)
		(layer "F.Fab")
		(uuid "671f41d0-6120-408a-a0ef-e1f19045b204")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "08c84f41-66bd-427e-86c4-39b62422f8ea")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "20d92517-c74e-44cc-b4b5-bb5f4d3c317f")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5b0c1c54-e717-4d7e-9783-d83491f515c4")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "DF_Comment" "2.54绿色单排排针-4P"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "b4a13315-7d5d-423d-80ea-23444e0f1076")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f4ae1114-127b-482f-8f1f-87361c76f8f4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.33 -1.33)
		(end 0 -1.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "75a43a52-60fb-4d86-817a-cc3d28573bef")
	)
	(fp_line
		(start -1.33 0)
		(end -1.33 -1.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "bf5dffbd-0bb4-4efe-bba9-bd9c9f1d2fc3")
	)
	(fp_line
		(start -1.33 1.27)
		(end -1.33 8.95)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "50015df9-8374-45c7-bc31-5d9ddf7b225e")
	)
	(fp_line
		(start -1.33 1.27)
		(end 1.33 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8a58a8d5-08e0-4d92-b579-52d57bdd4815")
	)
	(fp_line
		(start -1.33 8.95)
		(end 1.33 8.95)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "be1556de-51f6-4c71-ab05-f9e1f9260949")
	)
	(fp_line
		(start 1.33 1.27)
		(end 1.33 8.95)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3ae357a6-63b7-42ec-b52e-9f7e2bffd387")
	)
	(fp_line
		(start -1.8 -1.8)
		(end -1.8 9.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6e7b4eb1-fa19-4c0e-92e3-dffac1cc31e3")
	)
	(fp_line
		(start -1.8 9.4)
		(end 1.8 9.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4be1c3a2-3707-4e8b-a03e-8c2668a1788a")
	)
	(fp_line
		(start 1.8 -1.8)
		(end -1.8 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "26c9635b-aba6-4f2e-927b-5daf30bee67e")
	)
	(fp_line
		(start 1.8 9.4)
		(end 1.8 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "cff55cf9-2d36-49a1-8e1e-56f8449eab9e")
	)
	(fp_line
		(start -1.27 -0.635)
		(end -0.635 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7d5b960a-c0ca-44f5-a09b-8fc1993a57b3")
	)
	(fp_line
		(start -1.27 8.89)
		(end -1.27 -0.635)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "094c37b9-9441-4a8e-9d04-bfa5f395f759")
	)
	(fp_line
		(start -0.635 -1.27)
		(end 1.27 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "37ef5c80-cee5-4858-a725-4e4e54083bde")
	)
	(fp_line
		(start 1.27 -1.27)
		(end 1.27 8.89)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5b5c6ead-8410-45bf-b53c-a06690dc7e88")
	)
	(fp_line
		(start 1.27 8.89)
		(end -1.27 8.89)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1ad17a6e-6957-4288-8d31-ab5f20a7e6d6")
	)
	(fp_text user "${REFERENCE}"
		(at 0 3.81 90)
		(layer "F.Fab")
		(uuid "aa2e7306-9b7b-41c3-ae53-f2e0f67c0dfc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "aff07f09-86bd-4557-a96c-2d7be03fa92e")
	)
	(pad "2" thru_hole oval
		(at 0 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "bc019a12-7996-4eb7-a1d4-ee32ca56f2b5")
	)
	(pad "3" thru_hole oval
		(at 0 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "9a52991f-b5f7-46d3-ac46-530c7d5338f9")
	)
	(pad "4" thru_hole oval
		(at 0 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "dc54e4bd-c85c-4c17-8fc2-c949565eefe6")
	)
	(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)