(footprint "R_0603_1608Metric"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "resistor")
	(property "Reference" "REF**"
		(at 1.92 0 0)
		(layer "F.SilkS")
		(uuid "a09f3f90-8951-4bf3-8fa8-71d658f487c6")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "6V/50mA"
		(at 0 1.43 0)
		(layer "F.Fab")
		(uuid "e4fc61f2-9965-4069-89ec-1e4089be9ba7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1f331d5b-5617-45c8-89dc-5c8120f5e3a1")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4cac37d7-12ce-4c4a-9c2e-36f1881748b8")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "eb8a6ac4-f91d-4eed-92ea-bf657294438c")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" "https://item.szlcsc.com/8530937.html"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "208d6669-adea-4e65-9323-81ab04efeac4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "0603贴片自恢复保险丝0.05A/6V-0603L005/6AR"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "f273ee5e-fb16-4a57-831a-a05a936f3e59")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" "R0805"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "9a77f560-ecaa-48b5-850a-ec79f856ddd0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4bfedfd7-f184-408f-9e7d-75c752f4f69d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.237258 -0.5225)
		(end 0.237258 -0.5225)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "497ca3f8-295b-499b-9ead-11a8a7408d1b")
	)
	(fp_line
		(start -0.237258 0.5225)
		(end 0.237258 0.5225)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e5994407-5e5a-43e7-a67a-ceb960fe4e5e")
	)
	(fp_line
		(start -1.48 -0.73)
		(end 1.48 -0.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "cf9def01-621a-4eed-a4b3-b2cfd5987ec9")
	)
	(fp_line
		(start -1.48 0.73)
		(end -1.48 -0.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b071a1e3-57bd-4f2a-a273-705d4f87348b")
	)
	(fp_line
		(start 1.48 -0.73)
		(end 1.48 0.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "eb778125-e66a-4efb-be0e-b703944c3a25")
	)
	(fp_line
		(start 1.48 0.73)
		(end -1.48 0.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "41b120c7-60ba-4ee5-8414-3910d16e0fd9")
	)
	(fp_line
		(start -0.8 -0.4125)
		(end 0.8 -0.4125)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1437f428-56d2-4a61-b0bd-7d16b240a89a")
	)
	(fp_line
		(start -0.8 0.4125)
		(end -0.8 -0.4125)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6849a331-5a1f-4209-9e84-66a48dd6652c")
	)
	(fp_line
		(start 0.8 -0.4125)
		(end 0.8 0.4125)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "72c5c401-0c66-4ec1-b07c-04cc224720c5")
	)
	(fp_line
		(start 0.8 0.4125)
		(end -0.8 0.4125)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "45e7ba1c-2e80-4dd0-ac3c-bdd50f5d4cc5")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "c8f5db74-954d-471f-b670-8738836d40ac")
		(effects
			(font
				(size 0.4 0.4)
				(thickness 0.06)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "57c75a99-ce04-46ed-bddd-6d56ee60c376")
	)
	(pad "2" smd roundrect
		(at 0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "d09b5e41-75aa-4e9c-a668-31e040cf31cc")
	)
	(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)