(footprint "C_0402_1005Metric"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "capacitor")
	(property "Reference" "REF**"
		(at -1.835 -0.14 180)
		(layer "F.SilkS")
		(uuid "00647d34-30b7-4c16-9994-b93bc0ce60e1")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "10uF/10V"
		(at 0 1.16 180)
		(layer "F.Fab")
		(uuid "89174dd8-d679-46d9-94ad-2dc4446aa819")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cad49be8-6cd4-4083-831b-4f31614d60e3")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e52817c9-8ad4-4007-a39c-70c1d1d35146")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e07aa13f-b131-412e-9fb4-611abdab6d42")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "b2579249-b13f-4885-bd1e-d103921ab65f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "贴片电容0402-10UF-10V-X5R_GRM155R61A106ME44D"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "07a84d09-f2ff-4e59-9201-886d8e76d9af")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" "C0402"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "8be2406d-cbc2-4cff-859c-19c3f034b83a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d5f1b9d2-9823-4810-9336-63e28cf520cf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.107836 -0.36)
		(end 0.107836 -0.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "db4e3281-71bc-4f35-ad11-76fd0a6c4391")
	)
	(fp_line
		(start -0.107836 0.36)
		(end 0.107836 0.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "75432fac-c78f-4bcf-96bd-1ae838f37390")
	)
	(fp_line
		(start -0.91 -0.46)
		(end 0.91 -0.46)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "374f1616-265a-4b9d-8559-9f42eafff6d3")
	)
	(fp_line
		(start -0.91 0.46)
		(end -0.91 -0.46)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4314a0e6-dafa-4791-98fa-11ea5cef5c52")
	)
	(fp_line
		(start 0.91 -0.46)
		(end 0.91 0.46)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8c3d1cad-a59f-45aa-aaa8-148615d01077")
	)
	(fp_line
		(start 0.91 0.46)
		(end -0.91 0.46)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4cbedefa-a770-4941-95c6-d17e893d33d2")
	)
	(fp_line
		(start -0.5 -0.25)
		(end 0.5 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "13ecf289-f21e-47ce-9773-9f261efadecc")
	)
	(fp_line
		(start -0.5 0.25)
		(end -0.5 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b6c691b9-63e9-4b58-8140-e9ca86477cfe")
	)
	(fp_line
		(start 0.5 -0.25)
		(end 0.5 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f3a23c81-ec63-4343-aa96-cf08a12ba80e")
	)
	(fp_line
		(start 0.5 0.25)
		(end -0.5 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8207a633-a455-476e-a3e3-793b933a2dfa")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "86d7563e-5e87-4f24-a1cf-3c0a5fb4fd2b")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.04)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.48 0)
		(size 0.56 0.62)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "12c43743-e2f2-4390-a90c-7db5483ffcec")
	)
	(pad "2" smd roundrect
		(at 0.48 0)
		(size 0.56 0.62)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "8bcb29da-15ea-4f14-8c7f-84b3e41383f3")
	)
	(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)