(footprint "R_0805_2012Metric"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "resistor")
	(property "Reference" "REF**"
		(at 2.0925 -0.010001 90)
		(layer "F.SilkS")
		(uuid "7cdc8905-3810-4faa-be6b-27d0952ea19b")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "6V/2A"
		(at 0 1.65 0)
		(layer "F.Fab")
		(uuid "f11674d7-3539-4b23-ba87-a4e6b7c631f6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4963c45b-4ab9-4f82-85d7-b8b24ad91a63")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7252fdc2-030b-4db1-abc5-b6e1ed9fd06e")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7d516a9a-2c83-4864-b223-5046bb48cf4c")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" "https://item.szlcsc.com/947787.html"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "daa9013d-7e67-4b8f-b354-9b51aa421b1f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "0805贴片自恢复保险丝2A/6V-BSMD0805L-200"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "fcab2521-3541-44d7-9d49-c1c1aaa3f6a0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" "R0805"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "b7cdedaa-7285-420b-95cb-0228f9bb50eb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0abe8098-a0e9-419a-a0f3-0a3844df6dc4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.227064 -0.735)
		(end 0.227064 -0.735)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "82b80242-46f8-400b-89fa-28dd52ef7e34")
	)
	(fp_line
		(start -0.227064 0.735)
		(end 0.227064 0.735)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2c681b2c-e2a9-49f4-ba07-fad7bed6100a")
	)
	(fp_line
		(start -1.68 -0.95)
		(end 1.68 -0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4ba6f1c7-97ca-4191-b701-f5f07a9d221d")
	)
	(fp_line
		(start -1.68 0.95)
		(end -1.68 -0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "beea5a54-cd6d-4942-adbc-32cb3e5f9069")
	)
	(fp_line
		(start 1.68 -0.95)
		(end 1.68 0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fd15f30c-2aaa-4c06-983e-f4e5facebce6")
	)
	(fp_line
		(start 1.68 0.95)
		(end -1.68 0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "74b03498-5862-4a7e-bca5-f5a2a7c9235f")
	)
	(fp_line
		(start -1 -0.625)
		(end 1 -0.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8433b3ad-5e55-46f3-afdf-ee871ca81c40")
	)
	(fp_line
		(start -1 0.625)
		(end -1 -0.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6a109109-925d-4eca-8f76-d19d9ecd450e")
	)
	(fp_line
		(start 1 -0.625)
		(end 1 0.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2f9b989d-e5a5-4645-ab43-1d45ec4c1a69")
	)
	(fp_line
		(start 1 0.625)
		(end -1 0.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "85f32bf6-6aea-460d-bfa3-e447f0223958")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "cfb30f03-7aa3-456e-a457-3979589a7190")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.08)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.9125 0)
		(size 1.025 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.243902439)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "83912a85-bfa4-440a-8347-23854eb53128")
	)
	(pad "2" smd roundrect
		(at 0.9125 0)
		(size 1.025 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.243902439)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c6a5688b-7157-43c7-b87f-1633e106bef7")
	)
	(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)