(footprint "ESSOP-10-1EP_3.9x5mm_P1.0mm_EP3.2x2.3"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 3.71 1.78 -90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "250a4719-6d86-4a0a-a337-8a9935670d9d")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "CH224K"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c6bd512c-17a0-4227-8c9b-9636c0dcad44")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Library:ESSOP-10-1EP_3.9x5mm_P1.0mm_EP3.2x2.3"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "79c20b32-e825-4673-b2be-932d23ea55ed")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2c870988-eabf-4c56-90f3-850e5c5c4360")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1a390bb1-0bee-43de-b512-f50366ff7ddc")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" ""
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "984f3a20-e0a6-41ea-884b-fd81ea82cef6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "USB PD等快充协议受电芯片-CH224K-ESSOP10"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "96c83902-e7d3-41f8-b989-c8249b7f5e2a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "a9b4d8b0-9cbc-4861-aa7c-4b362c452f1c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "01701279-d339-4bfb-9b14-1c974bb5fd5e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -1.94 -2.5)
		(end 1.96 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "2aba397f-e5d2-4ce1-afb4-ed3f2abd749e")
	)
	(fp_circle
		(center -2.18 -2.71)
		(end -1.959773 -2.71)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "9e1342cd-bdf8-4155-a7d2-9dc6455a65d8")
	)
	(fp_line
		(start -3.35 -2.7)
		(end -3.35 2.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "29178cad-8223-48cd-97e9-8082a87d4282")
	)
	(fp_line
		(start -3.35 -2.7)
		(end 3.35 -2.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "bb171db5-122b-454a-8f1c-6b2702e6d08c")
	)
	(fp_line
		(start -3.35 2.7)
		(end 3.35 2.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "af55df79-5116-4543-aee3-f647f146de75")
	)
	(fp_line
		(start 3.35 -2.7)
		(end 3.35 2.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "61ccfb7b-7a64-4906-9b96-317a1d8cecef")
	)
	(fp_rect
		(start -1.95 -2.5)
		(end 1.95 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "1a1f5173-6319-4727-9f2a-0e94cfee7afc")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "172d307c-e61e-40b5-9d8c-0c41c624673e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0.12 -3.47 0)
		(layer "F.Fab")
		(uuid "f76dfe14-4a83-40cc-98dc-885b7813df4d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "0" smd rect
		(at 0 0)
		(size 2.3 3.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "ab37417f-9ff2-4da3-ae01-72ff215312fb")
	)
	(pad "1" smd rect
		(at -2.55 -2)
		(size 1.1 0.51)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "46a7f00b-7e17-40e9-9ff0-edeb584eacba")
	)
	(pad "2" smd rect
		(at -2.55 -1)
		(size 1.1 0.51)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "9e6e8554-aaa4-4b28-843b-f79b273e9d40")
	)
	(pad "3" smd rect
		(at -2.55 0)
		(size 1.1 0.51)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "5c9e5554-34a9-46ac-907b-511ae0dba3dc")
	)
	(pad "4" smd rect
		(at -2.55 1)
		(size 1.1 0.51)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "93005880-4c93-4d8a-a1fd-290a78f7242a")
	)
	(pad "5" smd rect
		(at -2.55 2)
		(size 1.1 0.51)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "bf3de9ae-86e1-4c8a-9668-991fbfa5f29e")
	)
	(pad "6" smd rect
		(at 2.55 2)
		(size 1.1 0.51)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "13d1b04f-05dd-4187-aa12-a77d29aa0903")
	)
	(pad "7" smd rect
		(at 2.55 1)
		(size 1.1 0.51)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c33d7cb5-5ff0-4ef6-bc16-85c9bc9d1e75")
	)
	(pad "8" smd rect
		(at 2.55 0)
		(size 1.1 0.51)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "34cef880-b100-472f-b083-10228508b66d")
	)
	(pad "9" smd rect
		(at 2.55 -1)
		(size 1.1 0.51)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "5f477702-b640-4527-9882-142c392edc87")
	)
	(pad "10" smd rect
		(at 2.55 -2)
		(size 1.1 0.51)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "539f4874-3825-441b-b620-6500b79da042")
	)
	(model "D:/download_LCEDA_3D_Model/ESSOP-10.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
)