(footprint "R_0402_1005Metric"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "resistor")
	(property "Reference" "REF**"
		(at -1.820261 -0.955 0)
		(layer "F.SilkS")
		(uuid "108675f7-487a-447e-8755-91841e939493")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "10K/1%"
		(at 0 1.17 0)
		(layer "F.Fab")
		(uuid "41fa9155-5390-4379-9d55-10c929af6584")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c53495b5-8f2a-456d-adb2-bb8530d83a09")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6677e99a-9490-49ec-b2a1-279f1c4ed169")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "68934e3a-a291-4cc5-8653-ccc09fd4e236")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "1bcdb22b-648d-4318-9b28-179e95139074")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "贴片电阻0402-10K-1%"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "cdd20fad-4eb0-425a-b5a5-59357c261739")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "ee286280-100d-46af-a06a-ad7a94464b8f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7d6291b6-6c7f-411d-87fa-e836f66898b9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -0.1 -0.27)
		(end 0.1 0.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "ef2b7ef9-7d6c-4e68-b740-a2d30d6bad08")
	)
	(fp_line
		(start -0.93 -0.47)
		(end 0.93 -0.47)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e405fea7-b4f1-4dad-a50d-0f9d70bed3a4")
	)
	(fp_line
		(start -0.93 0.47)
		(end -0.93 -0.47)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9e3f237a-a810-4a84-8552-959731bcf4de")
	)
	(fp_line
		(start 0.93 -0.47)
		(end 0.93 0.47)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a9069e4c-a29c-481e-a4cb-0d587f996e88")
	)
	(fp_line
		(start 0.93 0.47)
		(end -0.93 0.47)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "85c333bc-5919-4def-b4bd-081d25b9434b")
	)
	(fp_line
		(start -0.525 -0.27)
		(end 0.525 -0.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1330ab57-7868-4960-a35e-5b55d5fc8aaf")
	)
	(fp_line
		(start -0.525 0.27)
		(end -0.525 -0.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "565e16ba-10ac-4b37-94db-03edd14567e2")
	)
	(fp_line
		(start 0.525 -0.27)
		(end 0.525 0.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4d7405cb-4c77-46ee-998e-11025cd60071")
	)
	(fp_line
		(start 0.525 0.27)
		(end -0.525 0.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5b149815-e82c-486d-b159-b52d86c4939a")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "de06f10c-e53d-4af8-81d0-7dd72d311c3f")
		(effects
			(font
				(size 0.26 0.26)
				(thickness 0.04)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.51 0)
		(size 0.54 0.64)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "3450b4ce-a5b6-4c5e-add1-f3333fa355f8")
	)
	(pad "2" smd roundrect
		(at 0.51 0)
		(size 0.54 0.64)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c02ae2de-baec-4ab4-8bf1-60ac07b4c27f")
	)
	(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)