(footprint "USB_C_Receptacle_G-Switch_GT-USB-7010ASV"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "USB Type C, right-angle, SMT, https://datasheet.lcsc.com/lcsc/2204071530_G-Switch-GT-USB-7010ASV_C2988369.pdf")
	(tags "USB C Type-C Receptacle SMD")
	(property "Reference" "REF**"
		(at -2.93 -5.33 0)
		(layer "F.SilkS")
		(uuid "c428c8ea-5c56-470e-9353-6375e1d7b01b")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "USB_C_Receptacle_USB2.0"
		(at 0 5 0)
		(layer "F.Fab")
		(uuid "0e2543e3-3c21-4cf8-8fd1-8864d8e76016")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_USB:USB_C_Receptacle_G-Switch_GT-USB-7010ASV"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b19daba8-5dc6-4831-bd62-8b3527a27153")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0a0e0239-f2c2-402e-b0ad-fae18b44af84")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "79745f22-299a-4d75-a2fc-eeb020a0a747")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b1e05015-575b-4d72-80be-9d6f21047b79")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "USB-Type-C卧式贴片母座(TYPE-C-31-M-12)"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "80461d59-8538-4f9c-9d19-446f9b3e6f61")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "84ac7d24-ffce-481d-9c0c-b117a5f00121")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a7d44c6a-79c6-451e-8021-924fd33dd38e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -4.58 -1.85)
		(end -4.58 0.07)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1271a34f-14c6-4b88-9ff3-648611c15aa5")
	)
	(fp_line
		(start -4.58 3.785)
		(end -4.58 2.08)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "32b00785-9ca7-49d7-9829-07719db46dfd")
	)
	(fp_line
		(start 4.58 0.07)
		(end 4.58 -1.85)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e72c6c02-e899-4fd7-8de9-2667de05be06")
	)
	(fp_line
		(start 4.58 2.08)
		(end 4.58 3.785)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ed10ee40-d968-4e5c-9772-20d03d8b8e77")
	)
	(fp_line
		(start 4.58 3.785)
		(end -4.58 3.785)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8143a9ac-0d02-4b26-b6ab-1d7bebdc9389")
	)
	(fp_line
		(start -5.32 -4.85)
		(end 5.32 -4.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "de436832-e927-4c57-a6cc-663eb27d0fad")
	)
	(fp_line
		(start -5.32 4.18)
		(end -5.32 -4.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "66509646-2ef0-47c4-b072-c06e4aed4517")
	)
	(fp_line
		(start 5.32 -4.85)
		(end 5.32 4.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8c26c30d-e310-41d8-9d9f-55a15b23a249")
	)
	(fp_line
		(start 5.32 4.18)
		(end -5.32 4.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2320cab1-55e7-4cc4-bb07-c61ba9612b64")
	)
	(fp_line
		(start -4.47 -3.675)
		(end -4.47 3.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d0d24eeb-a3fb-4114-90c7-39851df8f517")
	)
	(fp_line
		(start -4.47 -3.675)
		(end 4.47 -3.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "40457b60-8502-4385-b9d8-9de001ab3285")
	)
	(fp_line
		(start -4.47 3.675)
		(end 4.47 3.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0f21ea93-19e4-4d24-a0e3-b012be6977cf")
	)
	(fp_line
		(start 4.47 3.675)
		(end 4.47 -3.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "53339168-a0e1-4391-b5ee-2a7b3bd73588")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "e41b064c-482b-4f35-86f9-6f4ecda67f35")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -2.89 -2.605)
		(size 0.65 0.65)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(uuid "13112687-8669-4c42-83a4-ec38c3f99810")
	)
	(pad "" np_thru_hole circle
		(at 2.89 -2.605)
		(size 0.65 0.65)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(uuid "e50696fc-d39e-4c08-ab27-8394dbeb20d9")
	)
	(pad "A1" smd rect
		(at -3.2 -3.725)
		(size 0.6 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "d44c8896-70e6-4a8d-ab10-a4f762461d51")
	)
	(pad "A4" smd rect
		(at -2.4 -3.725)
		(size 0.6 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "20f23a71-1c56-428b-86ee-462de38fe4d4")
	)
	(pad "A5" smd rect
		(at -1.25 -3.725)
		(size 0.3 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "b606b20f-7b36-4c31-9d4a-f85d9dcf86a2")
	)
	(pad "A6" smd rect
		(at -0.25 -3.725)
		(size 0.3 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "2bc5550b-81c3-4f89-8ea2-41aa20bd66a0")
	)
	(pad "A7" smd rect
		(at 0.25 -3.725)
		(size 0.3 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "516ef9e2-98ff-4105-8e81-08f3fe72e800")
	)
	(pad "A8" smd rect
		(at 1.25 -3.725)
		(size 0.3 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "81d92904-ac0f-42e1-a3b2-ce700764a7a4")
	)
	(pad "A9" smd rect
		(at 2.4 -3.725)
		(size 0.6 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "42399557-4188-445b-a1a4-981e98c79443")
	)
	(pad "A12" smd rect
		(at 3.2 -3.725)
		(size 0.6 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "eae209cd-b830-43b8-bc70-46e9bfba2c57")
	)
	(pad "B1" smd rect
		(at 3.2 -3.725)
		(size 0.6 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "b50350cb-fb2a-493e-81e7-96b6a17ae921")
	)
	(pad "B4" smd rect
		(at 2.4 -3.725)
		(size 0.6 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "e6895b3e-7de5-4286-a6ec-963c2fe79b71")
	)
	(pad "B5" smd rect
		(at 1.75 -3.725)
		(size 0.3 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "5b3f5ed0-7dbb-49d2-8087-92f2f270e161")
	)
	(pad "B6" smd rect
		(at 0.75 -3.725)
		(size 0.3 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "2eb4dcde-ce74-49a8-9494-48a3913f03a8")
	)
	(pad "B7" smd rect
		(at -0.75 -3.725)
		(size 0.3 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "f633d4ab-33c4-43ff-80ae-5fec182a3336")
	)
	(pad "B8" smd rect
		(at -1.75 -3.725)
		(size 0.3 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "0c4dc15d-7861-4bac-b3cd-3f2aa2b5d0aa")
	)
	(pad "B9" smd rect
		(at -2.4 -3.725)
		(size 0.6 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "cb7727a6-72a8-4915-9cf4-eded74f66d66")
	)
	(pad "B12" smd rect
		(at -3.2 -3.725)
		(size 0.6 1.24)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "fae86222-be8c-42eb-b94a-7ace6b9d6f89")
	)
	(pad "S1" thru_hole oval
		(at -4.32 -3.125)
		(size 1 2.1)
		(drill oval 0.6 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "7518ae7d-0441-4a9e-936e-5ce58a430fa1")
	)
	(pad "S1" thru_hole oval
		(at -4.32 1.075)
		(size 1 1.8)
		(drill oval 0.6 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "a4eb121e-a8fc-4264-b6f2-cdaed8d65755")
	)
	(pad "S1" thru_hole oval
		(at 4.32 -3.125)
		(size 1 2.1)
		(drill oval 0.6 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "862461b3-6f8f-4f02-a067-814ae4bf7007")
	)
	(pad "S1" thru_hole oval
		(at 4.32 1.075)
		(size 1 1.8)
		(drill oval 0.6 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "fb9cf5fa-c3db-4cd7-968d-bce18f47d7b2")
	)
	(model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_G-Switch_GT-USB-7010ASV.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "D:/download_LCEDA_3D_Model/USB-C_SMD-TYPE-C-31-M-026.step"
		(offset
			(xyz 0 -1 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 -180)
		)
	)
)