(footprint "QFN-32-1EP_4x4mm_P0.4mm_EP2.65x2.65mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "QFN, 32 Pin (https://www.renesas.com/eu/en/package-image/pdf/outdrawing/l32.4x4a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at -3.059739 0.825 -90)
		(layer "F.SilkS")
		(uuid "bdc90593-0cdc-4d2c-8fa5-c8901eb000a3")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "RTL8111H-CG-RH"
		(at 0 3.3 0)
		(layer "F.Fab")
		(uuid "b973c9c3-9211-42ee-9989-09200a3a7be6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_4x4mm_P0.4mm_EP2.65x2.65mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d425373c-d05b-4874-a681-b3e3d70d4be3")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6ccc258f-e804-435d-a2ab-7b721c224a8f")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b48b567f-38b2-46ac-a655-22e039869240")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" ""
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "735ccecb-bc18-4137-8f9a-2b5ec2c16e53")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "以太网控制器IC-RTL8111H-CG-RH(PCIE-LAN)-QFN32"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "0c7da015-a20b-4c73-b1b5-600c627d71a7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "8891dc52-f83a-4ded-993b-c9f2d5e44cb5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6af743cf-b263-42a4-96be-8120eaf6e6cc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.11 2.11)
		(end -2.11 1.76)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "71fcbbcf-35f4-4656-99a7-e38c70555719")
	)
	(fp_line
		(start -1.76 -2.11)
		(end -2.11 -2.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "98f7319c-8cc6-4916-9bf4-c1ce094bdbeb")
	)
	(fp_line
		(start -1.76 2.11)
		(end -2.11 2.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7b25c9ff-8fa5-4733-b3df-b3d60e09948b")
	)
	(fp_line
		(start 1.76 -2.11)
		(end 2.11 -2.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7583dda2-2579-4343-bb2b-0112ff07f062")
	)
	(fp_line
		(start 1.76 2.11)
		(end 2.11 2.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fcdd1631-c41c-4d8d-a001-bc377784a768")
	)
	(fp_line
		(start 2.11 -2.11)
		(end 2.11 -1.76)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8b71cf8c-09af-4355-b25f-38c669969528")
	)
	(fp_line
		(start 2.11 2.11)
		(end 2.11 1.76)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "eb8511e9-b317-4379-9655-e0d99e5c7942")
	)
	(fp_circle
		(center -1.935 -2.11)
		(end -1.683355 -2.11)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "b3973e32-983c-4970-b826-1ab290bd6012")
	)
	(fp_line
		(start -2.6 -2.6)
		(end -2.6 2.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "069daeff-04e6-4859-895c-f94e7310262d")
	)
	(fp_line
		(start -2.6 2.6)
		(end 2.6 2.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6d504a76-e8f6-4e81-94bc-b82d63fdb11c")
	)
	(fp_line
		(start 2.6 -2.6)
		(end -2.6 -2.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1f1cb529-c677-4362-b700-d1c8e7307029")
	)
	(fp_line
		(start 2.6 2.6)
		(end 2.6 -2.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "138767fd-a3c0-4968-a4ba-7014deb8481d")
	)
	(fp_line
		(start -2 -1)
		(end -1 -2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5687674c-0e2f-40ea-8f56-bf42f7ed57cd")
	)
	(fp_line
		(start -2 2)
		(end -2 -1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8e0ba0e5-8eef-49de-b3e9-99c8e921103c")
	)
	(fp_line
		(start -1 -2)
		(end 2 -2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8fd8e96e-81c4-4ee7-8aec-6d89dbeead56")
	)
	(fp_line
		(start 2 -2)
		(end 2 2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b04f1275-a36b-4e34-90b9-793e10b71a3b")
	)
	(fp_line
		(start 2 2)
		(end -2 2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "afbbe0aa-35b5-413f-a7d1-6fc3e3e931c5")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "2e530c53-fab4-48f7-8028-a5a32ba54166")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" smd roundrect
		(at -0.66 -0.66)
		(size 1.07 1.07)
		(layers "F.Paste")
		(roundrect_rratio 0.2336448598)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "862486cc-9354-45b1-987d-e62d6484a65d")
	)
	(pad "" smd roundrect
		(at -0.66 0.66)
		(size 1.07 1.07)
		(layers "F.Paste")
		(roundrect_rratio 0.2336448598)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "5d598103-db3f-4e1b-84c4-f30fc2eb727b")
	)
	(pad "" smd roundrect
		(at 0.66 -0.66)
		(size 1.07 1.07)
		(layers "F.Paste")
		(roundrect_rratio 0.2336448598)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "0a8165f5-a005-458e-98df-a89a650527c5")
	)
	(pad "" smd roundrect
		(at 0.66 0.66)
		(size 1.07 1.07)
		(layers "F.Paste")
		(roundrect_rratio 0.2336448598)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "1af4311f-c6e1-43a7-bfc5-6b2af11c1567")
	)
	(pad "1" smd custom
		(at -1.95 -1.4)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.35 0.020711) (xy 0.35 0.05) (xy -0.35 0.05) (xy -0.35 -0.05) (xy 0.279289 -0.05)
				)
				(width 0.1)
				(fill yes)
			)
		)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "a4f925ab-030f-437d-83fa-a8a065bdad95")
	)
	(pad "2" smd roundrect
		(at -1.95 -1)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "37286a8d-747b-4c1b-aa58-27311c6bcefd")
	)
	(pad "3" smd roundrect
		(at -1.95 -0.6)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "bdcbf2e3-516a-4ec4-9837-12c199a1b858")
	)
	(pad "4" smd roundrect
		(at -1.95 -0.2)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "d1b32cc6-3e1e-4519-93aa-4fa4c9730963")
	)
	(pad "5" smd roundrect
		(at -1.95 0.2)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "b15aa25c-9050-4ac1-83c9-84e1ae706c81")
	)
	(pad "6" smd roundrect
		(at -1.95 0.6)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "307cf1cd-a4be-4b0c-9208-24f11c6c70cf")
	)
	(pad "7" smd roundrect
		(at -1.95 1)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "f2a90ccf-82ef-4530-b182-ce045109c339")
	)
	(pad "8" smd custom
		(at -1.95 1.4)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.35 -0.020711) (xy 0.279289 0.05) (xy -0.35 0.05) (xy -0.35 -0.05) (xy 0.35 -0.05)
				)
				(width 0.1)
				(fill yes)
			)
		)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "43c150d4-7e69-4ec1-857e-026bf576a84a")
	)
	(pad "9" smd custom
		(at -1.4 1.95)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.05 0.35) (xy -0.05 0.35) (xy -0.05 -0.279289) (xy 0.020711 -0.35) (xy 0.05 -0.35)
				)
				(width 0.1)
				(fill yes)
			)
		)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "b7a4aa73-0b34-4db3-840f-36cce15af564")
	)
	(pad "10" smd roundrect
		(at -1 1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "e9452065-6c87-490b-96a8-f8d0bda34fe7")
	)
	(pad "11" smd roundrect
		(at -0.6 1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "09df6592-8890-425b-888f-68832c3cca1e")
	)
	(pad "12" smd roundrect
		(at -0.2 1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "70e0dd77-0aee-432a-95d2-3f0da0ee21aa")
	)
	(pad "13" smd roundrect
		(at 0.2 1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "b27603fc-3543-4691-a38e-ac059a67ba83")
	)
	(pad "14" smd roundrect
		(at 0.6 1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "b6aa50cd-810c-4daa-9d82-fe21a98f6700")
	)
	(pad "15" smd roundrect
		(at 1 1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "db98deef-0262-4470-a82f-d79bce6b1386")
	)
	(pad "16" smd custom
		(at 1.4 1.95)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.05 -0.279289) (xy 0.05 0.35) (xy -0.05 0.35) (xy -0.05 -0.35) (xy -0.020711 -0.35)
				)
				(width 0.1)
				(fill yes)
			)
		)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "966b4768-23b9-4d44-940b-5619c297547d")
	)
	(pad "17" smd custom
		(at 1.95 1.4)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.35 0.05) (xy -0.279289 0.05) (xy -0.35 -0.020711) (xy -0.35 -0.05) (xy 0.35 -0.05)
				)
				(width 0.1)
				(fill yes)
			)
		)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "940d340c-27a8-40c3-85fd-859b7769bb59")
	)
	(pad "18" smd roundrect
		(at 1.95 1)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "7b90cb43-ba58-42c9-9810-364682eb0f8e")
	)
	(pad "19" smd roundrect
		(at 1.95 0.6)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "5b9007ed-7b0e-4de5-bece-cd932eec197c")
	)
	(pad "20" smd roundrect
		(at 1.95 0.2)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "f286997b-3b2f-482d-9fa7-fdb46793d4ce")
	)
	(pad "21" smd roundrect
		(at 1.95 -0.2)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "5b30b30b-9261-4ae8-8324-2f5e66361124")
	)
	(pad "22" smd roundrect
		(at 1.95 -0.6)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "5d13a233-f648-4d0b-a1ec-acb19d3a2288")
	)
	(pad "23" smd roundrect
		(at 1.95 -1)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "fb70c98d-aa06-4eb1-b68b-e5f4e2920362")
	)
	(pad "24" smd custom
		(at 1.95 -1.4)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.35 0.05) (xy -0.35 0.05) (xy -0.35 0.020711) (xy -0.279289 -0.05) (xy 0.35 -0.05)
				)
				(width 0.1)
				(fill yes)
			)
		)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c1cb0f4b-fc0d-4d89-991f-4644a286a00d")
	)
	(pad "25" smd custom
		(at 1.4 -1.95)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.05 0.279289) (xy -0.020711 0.35) (xy -0.05 0.35) (xy -0.05 -0.35) (xy 0.05 -0.35)
				)
				(width 0.1)
				(fill yes)
			)
		)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "234a7cde-76ae-446f-a04e-623d794da904")
	)
	(pad "26" smd roundrect
		(at 1 -1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "541f6701-8858-4ef8-bb6d-7435bd3ee190")
	)
	(pad "27" smd roundrect
		(at 0.6 -1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "1b93e44c-afbb-45bc-835b-0eeddac0a8d9")
	)
	(pad "28" smd roundrect
		(at 0.2 -1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "3dd175fb-10b0-4dc8-9f8e-d18761f894f9")
	)
	(pad "29" smd roundrect
		(at -0.2 -1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "f47d7076-7c11-474d-90eb-a2e7c2061801")
	)
	(pad "30" smd roundrect
		(at -0.6 -1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c88e31f2-3298-41d1-8404-497d31972db7")
	)
	(pad "31" smd roundrect
		(at -1 -1.95)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "3ca89d74-60f7-4a1d-afb2-04fe19b5a310")
	)
	(pad "32" smd custom
		(at -1.4 -1.95)
		(size 0.129289 0.129289)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.05 0.35) (xy 0.020711 0.35) (xy -0.05 0.279289) (xy -0.05 -0.35) (xy 0.05 -0.35)
				)
				(width 0.1)
				(fill yes)
			)
		)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "d014bb67-b2b3-48a6-bf58-207108934623")
	)
	(pad "33" smd rect
		(at 0 0)
		(size 2.65 2.65)
		(layers "F.Cu" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "9b1f2cf7-639e-435b-90d9-84bb72dcb623")
	)
	(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-32-1EP_4x4mm_P0.4mm_EP2.65x2.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)