(footprint "Battery_Holder_CR1220_S8411-45R"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "S8411-45R_1")
	(tags "Connector")
	(property "Reference" "REF**"
		(at 2.36 9.65 -90)
		(layer "F.SilkS")
		(uuid "a66298b4-8259-47e1-b3f9-2064541ec473")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Battery_Cell"
		(at -0.412 -0.096 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "9b5052a6-047b-4924-ad68-65f36674ef1c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.254)
			)
		)
	)
	(property "Footprint" "Battery:Battery_Holder_CR1220_S8411-45R"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "52b66ac0-5ced-466e-be81-7a55139b01e4")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c0ddc64d-fa82-4834-a1ef-e3c58dc87e70")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cdbf1451-77a6-4eae-ba5f-ceb062b9b17d")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" "https://item.szlcsc.com/1049689.html"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "895d2a16-8d68-4d0e-b355-94ba5875351e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "CR1220电池底座_BS-12-B3AA003"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "b90de17d-c6be-47a2-873f-c264187dcfec")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "22bbb70f-a449-4e94-a409-1257e5408098")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "62987c99-03dc-4c06-ac02-c2a84ff33617")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -6.832 6.625)
		(end -3.27 6.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3cd73fcf-df85-4d65-87aa-dee6d01dc929")
	)
	(fp_line
		(start -6.832 8.307)
		(end -6.832 6.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f1f8a9b2-be9f-41df-ac6f-2401ee60e576")
	)
	(fp_line
		(start -6.832 8.307)
		(end -1.553 8.307)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2760419f-7735-4b0e-a555-38c63ded0ec8")
	)
	(fp_line
		(start 6.832 6.625)
		(end 3.296 6.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "28cd35f0-f8ff-4267-9fd4-01bf922de9b7")
	)
	(fp_line
		(start 6.832 8.307)
		(end 1.49 8.307)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7591e813-d1d9-4568-b1b4-740bc9e3e918")
	)
	(fp_line
		(start 6.832 8.307)
		(end 6.832 6.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "93b4ce37-7487-4fd4-a2d7-33bed8730f9a")
	)
	(fp_arc
		(start -3.295295 6.625783)
		(mid -7.399998 0.000879)
		(end -3.29687 -6.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "759a7d46-fcb4-483e-bf9e-82a6f3f7d742")
	)
	(fp_arc
		(start 3.295287 -6.625787)
		(mid 7.399995 -0.000884)
		(end 3.29687 6.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c4f779db-726a-4da6-b37c-ef0ba9d140f4")
	)
	(fp_line
		(start -6.832 6.625)
		(end -6.832 8.307)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "da0cc7be-3b22-434a-88e7-772798c47f81")
	)
	(fp_line
		(start -6.832 8.307)
		(end 6.832 8.307)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f48f4a5c-df10-47dc-984d-3a20592edcac")
	)
	(fp_line
		(start -3.29687 6.625)
		(end -6.832 6.625)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3dcb3855-7c44-41c9-84ea-e6d5ad63efb6")
	)
	(fp_line
		(start 6.832 6.625)
		(end 3.27 6.625)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "61a27e5b-0a23-4a62-b535-b1d5c2385b38")
	)
	(fp_line
		(start 6.832 8.307)
		(end 6.832 6.625)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "74496f8b-a912-4c8f-93c1-27019e5025be")
	)
	(fp_circle
		(center 0 0)
		(end 0 7.4)
		(stroke
			(width 0.2)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "dab86c68-8514-4755-b972-3383810e146e")
	)
	(fp_text user "${REFERENCE}"
		(at -0.412 -0.096 180)
		(layer "F.Fab")
		(uuid "ffaa42f8-2c61-4f3c-be10-212720aff2b0")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.254)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 -3.725)
		(size 1.05 1.05)
		(drill 1.05)
		(layers "*.Cu" "*.Mask")
		(uuid "4bf58f0c-bd52-4641-a28e-7ca2497837ee")
	)
	(pad "" np_thru_hole circle
		(at 0 3.725)
		(size 1.3 1.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(uuid "3fe0ebcc-4d94-47e9-8dc8-b1775a79f1a0")
	)
	(pad "1" smd rect
		(at 0 8.2)
		(size 2.3 4.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "eab935e3-9ec4-4903-be38-15cc704db71c")
	)
	(pad "2" smd rect
		(at 0 -8.2)
		(size 2.3 4.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "96ed5f4c-b905-4f2b-9099-7f2c351e0588")
	)
	(model "D:/项目/2023样品项目/LattePanda Mu/LIB_S8411-45R/S8411-45R/3D/S8411-45R.stp"
		(offset
			(xyz 0 -0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)