(footprint "Fuse_0805_2012Metric"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
	(tags "fuse")
	(property "Reference" "REF**"
		(at -1 -1.439998 90)
		(layer "F.SilkS")
		(uuid "f873ecf1-de81-451f-bd80-90822f35c5df")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "6V/1A"
		(at 0 1.65 0)
		(layer "F.Fab")
		(uuid "cb69ea2b-a7b8-420f-94d4-f3517fc6676f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Fuse:Fuse_0805_2012Metric"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "12d6775b-2753-4270-a834-b7181bc2364e")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b36439aa-4f35-49ed-8b30-9da82a611d8a")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4788ac9d-c92d-47f3-acb5-70ed88c4bd04")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" "https://item.szlcsc.com/947770.html"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "99ae7071-e6bd-4d3a-a455-8cc1456f5b50")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "0805贴片自恢复保险丝1A/6V-BSMD0805-100-6V"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "eccbb124-cce2-4d14-9871-cd2ea5b50361")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" "R0603"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "be2e3bf0-5d46-4318-908b-4869ebd4fcaf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8e23c39e-d8d8-4247-844f-80d24637f50a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.258578 -0.71)
		(end 0.258578 -0.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1c4db232-589e-411d-b89f-837b7fa3a713")
	)
	(fp_line
		(start -0.258578 0.71)
		(end 0.258578 0.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "48120c22-31c4-4287-b10c-5c389dbbfffd")
	)
	(fp_line
		(start -1.68 -0.95)
		(end 1.68 -0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7f0c1652-f4f5-4fe3-9a32-eac5d79642b7")
	)
	(fp_line
		(start -1.68 0.95)
		(end -1.68 -0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "0ef2beff-051c-4a15-a18e-dbac61e1448e")
	)
	(fp_line
		(start 1.68 -0.95)
		(end 1.68 0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9170fd26-46cd-41ee-a977-f38fbf2099df")
	)
	(fp_line
		(start 1.68 0.95)
		(end -1.68 0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5bf06c35-e3b9-4721-b605-3ead2af005c5")
	)
	(fp_line
		(start -1 -0.6)
		(end 1 -0.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2abdc108-2849-430f-bfe3-b9c070830e14")
	)
	(fp_line
		(start -1 0.6)
		(end -1 -0.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c984a7bc-ce54-4914-951b-86d48c066054")
	)
	(fp_line
		(start 1 -0.6)
		(end 1 0.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9696fdb2-77fa-4c09-8043-a9c37d49b79e")
	)
	(fp_line
		(start 1 0.6)
		(end -1 0.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4b75f0ec-fb0b-4436-807c-e5a3d1f8f05c")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "78ed1f48-889f-48b5-b224-14a8cf51fd68")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.08)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.9375 0)
		(size 0.975 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "9e4eb2be-abcb-4395-b7e1-42aa345ff090")
	)
	(pad "2" smd roundrect
		(at 0.9375 0)
		(size 0.975 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "97dd7470-32fb-4dbf-8320-3c41caf5f541")
	)
	(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)