(footprint "USB_A_CUI_UJ2-ADH-TH_Horizontal_Stacked"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "USB-A two stacked horizontal receptacle, through-hole (https://www.cuidevices.com/product/resource/uj2-adh-th.pdf)")
	(tags "USB-A CUI stacked horizontal through-hole")
	(property "Reference" "REF**"
		(at 5.197685 7.2 90)
		(layer "F.SilkS")
		(uuid "edcc631e-71e1-4044-b7e8-99a57154450a")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "USB_A_Stacked"
		(at -2.2 14.18 0)
		(layer "F.Fab")
		(uuid "729c28cf-bbb6-4b06-a15d-1cd121a7c60e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_USB:USB_A_CUI_UJ2-ADH-TH_Horizontal_Stacked"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "29578129-cedc-469a-aacc-a58232b5f60b")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" " ~"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "673fd23a-b84a-410b-8b6c-13ff62c74401")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "eeadc28f-69b3-40b8-a577-ce99c03636d2")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" ""
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "bd91bd37-0fd4-4e00-9242-3b7f6b07468e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "USB2.0-A型双层白胶母座"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "a8d7b10e-f5ca-4c53-b650-3331384b0a5c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "00938be5-e8ad-40b3-ad6c-348476e50ec3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "36093065-af97-4009-a3b6-51c2eb1addf2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -11.58 10.13)
		(end -4.73 10.13)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "df6bf15b-7945-444f-8653-0a052b6ecc01")
	)
	(fp_line
		(start -4.73 -3.13)
		(end -11.58 -3.13)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fbb8aa48-13af-4999-b235-47e1a1f3f934")
	)
	(fp_line
		(start -0.5 -3.75)
		(end 0 -3.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "244aff44-3c33-4e21-a06a-401f2e5955c9")
	)
	(fp_line
		(start 0 -3.25)
		(end 0.5 -3.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "99a9fa52-2d1a-4af9-b32a-b11bb5e613d1")
	)
	(fp_line
		(start 0.5 -3.75)
		(end -0.5 -3.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "683a0b9b-be97-4d19-ad3a-2b41acb6e821")
	)
	(fp_line
		(start 4.07 8.4)
		(end 4.07 -1.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c0cdac68-2440-4c7a-beed-7191cc818d84")
	)
	(fp_line
		(start -13.51 -4.55)
		(end -13.51 11.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3071bd72-11e1-45fb-b147-5d8f1eed126b")
	)
	(fp_line
		(start -13.51 -4.55)
		(end -12.21 -4.55)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e49d032d-25f7-4ebf-bf4c-395edce1e63b")
	)
	(fp_line
		(start -13.51 11.55)
		(end -12.21 11.55)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8ddcc2f5-dc0d-4455-a186-651cdffa7a0b")
	)
	(fp_line
		(start -12.21 -4.55)
		(end -12.21 -3.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a2ee495e-2b03-46e0-a21d-9cdb33b74b19")
	)
	(fp_line
		(start -12.21 10.5)
		(end -4.92 10.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "969bfedc-c658-4739-b668-14f6097d1e63")
	)
	(fp_line
		(start -12.21 11.55)
		(end -12.21 10.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "64b10aa4-a24d-4c20-9e19-927188b17fdf")
	)
	(fp_line
		(start -4.92 -3.5)
		(end -12.21 -3.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "17d30e67-7b33-4f09-83eb-28daf7ae7fa2")
	)
	(fp_line
		(start -0.5 -3.5)
		(end 0.76 -3.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "17ba58cb-29a3-43b4-9236-e56bcca940d3")
	)
	(fp_line
		(start -0.5 10.5)
		(end 0.76 10.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c56d2f0c-3d8f-4ad0-b62d-c857cb171276")
	)
	(fp_line
		(start 4.44 8.36)
		(end 4.44 -1.36)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1e8ee1b4-2542-496a-a21b-5c2843f4c556")
	)
	(fp_arc
		(start -4.92 -3.5)
		(mid -2.71 -5.321444)
		(end -0.5 -3.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "86986f54-7319-42fa-8688-6b88140fc157")
	)
	(fp_arc
		(start -0.5 10.5)
		(mid -2.71 12.321444)
		(end -4.92 10.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d96ffa3b-6ebb-4e40-8eeb-efdff0586945")
	)
	(fp_arc
		(start 0.76 -3.5)
		(mid 4.104741 -5.017595)
		(end 4.44 -1.36)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2bf76434-f5c9-46a5-86d9-1d5f8b3de174")
	)
	(fp_arc
		(start 2.97 10.07)
		(mid 2.97 10.07)
		(end 2.97 10.07)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9ab751ac-0142-4a93-bbdc-91c2eb228ed1")
	)
	(fp_arc
		(start 4.44 8.36)
		(mid 4.104744 12.017599)
		(end 0.76 10.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "da0f0f4b-ced9-4c0d-8489-c0ada93f9a57")
	)
	(fp_line
		(start -13.01 -3)
		(end -13.01 10)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8e03e017-4a74-49fb-aadb-f8465b6393b0")
	)
	(fp_line
		(start -13.01 10)
		(end 3.94 10)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f98bca1a-1269-4ef9-9aa1-d7fcd665a5af")
	)
	(fp_line
		(start -11.49 5.595)
		(end -11.49 7.405)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b25b3d46-df4a-434a-af6b-5b42464f9d4a")
	)
	(fp_line
		(start -11.49 7.405)
		(end -5.74 8.065)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "de8a45ad-1c64-4d8d-ada2-1ca69c708416")
	)
	(fp_line
		(start -11.46 -0.405)
		(end -11.46 1.405)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "34d7a480-13f9-4eda-852f-8d857e5984e1")
	)
	(fp_line
		(start -11.46 1.405)
		(end -5.71 2.065)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1ebc62f0-9e73-49ac-a976-a7094c2b6737")
	)
	(fp_line
		(start -5.74 4.935)
		(end -11.49 5.595)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fac462f6-61d8-4b1a-bab7-c56842a9cbcf")
	)
	(fp_line
		(start -5.74 8.065)
		(end -5.74 4.935)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c6d84eeb-25ce-4098-b4ea-b996c82b7c3e")
	)
	(fp_line
		(start -5.71 -1.065)
		(end -11.46 -0.405)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "aa0704cf-972a-40f5-b07a-6112077437bc")
	)
	(fp_line
		(start -5.71 2.065)
		(end -5.71 -1.065)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6b4b5a6b-2d12-42d8-a5fb-34f46adb6ba2")
	)
	(fp_line
		(start 0 -2.5)
		(end -0.5 -3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "87c5b9c3-ec00-410a-84f8-98736c8857b4")
	)
	(fp_line
		(start 0 -2.5)
		(end 0.5 -3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d08b2b15-7d5d-45eb-ae1f-678c8999e19d")
	)
	(fp_line
		(start 3.94 -3)
		(end -13.01 -3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1734b895-a264-4a93-b446-65bcd36e10d0")
	)
	(fp_line
		(start 3.94 10)
		(end 3.94 -3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "16ba51eb-b9dd-477b-ae7a-a1681d0b5963")
	)
	(fp_rect
		(start -13.01 -4.05)
		(end -12.71 -3)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "499f2604-a520-4c5e-b7eb-5120ee190e96")
	)
	(fp_rect
		(start -13.01 10)
		(end -12.71 11.05)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "bb8b1277-dd2d-47e1-be73-866b4cd7e250")
	)
	(fp_text user "${REFERENCE}"
		(at -4.535 3.5 0)
		(layer "F.Fab")
		(uuid "56fab04b-0d1e-413f-aca0-b61e7161ef91")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.5 1.5)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "e1acd9cf-3940-426b-b46b-aa84235b93de")
	)
	(pad "2" thru_hole circle
		(at 0 2.5)
		(size 1.5 1.5)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "8a06eae3-63b6-4ef1-82e9-be6bbd9dbd87")
	)
	(pad "3" thru_hole circle
		(at 0 4.5)
		(size 1.5 1.5)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "73dd24ac-6d64-465c-98e4-22ae8b9fc9da")
	)
	(pad "4" thru_hole circle
		(at 0 7)
		(size 1.5 1.5)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "72b8904e-df6d-4075-a9a3-1372b18b3a91")
	)
	(pad "5" thru_hole circle
		(at 2.62 0)
		(size 1.5 1.5)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "45cbb22b-719f-4cbf-9526-12f0bce39a09")
	)
	(pad "6" thru_hole circle
		(at 2.62 2.5)
		(size 1.5 1.5)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "d2713be4-b0f4-43d0-a915-e75518421ede")
	)
	(pad "7" thru_hole circle
		(at 2.62 4.5)
		(size 1.5 1.5)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "12e7aaf9-ab9f-4410-8c87-b9f4f8594974")
	)
	(pad "8" thru_hole circle
		(at 2.62 7)
		(size 1.5 1.5)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "f9a0b762-3630-44b3-a3b8-efd5d87578c7")
	)
	(pad "9" thru_hole circle
		(at -2.71 -3.07)
		(size 3.5 3.5)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "4c8ab65d-cc5d-4d6b-ac2c-ab56b57f4ab8")
	)
	(pad "9" thru_hole circle
		(at -2.71 10.07)
		(size 3.5 3.5)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "cc41de37-e973-4e59-b8f9-3714f8ac6a3b")
	)
	(pad "9" thru_hole circle
		(at 2.97 -3.07)
		(size 3.5 3.5)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "161b2840-462d-4998-80d4-9b8aa8322357")
	)
	(pad "9" thru_hole circle
		(at 2.97 10.07)
		(size 3.5 3.5)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "88d83298-3474-4fd8-af2e-0a14d705f5d2")
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_CUI_UJ2-ADH-TH_Horizontal_Stacked.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "D:/download_LCEDA_3D_Model/USB-A-TH_AF-SS-JB17.031.step"
		(offset
			(xyz -3.75 -3.5 3.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
)