(footprint "TestPoint_Pad_D1.5mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SMD pad as test Point, diameter 1.5mm")
	(tags "test point SMD pad")
	(property "Reference" "REF**"
		(at 0 -1.648 180)
		(layer "F.SilkS")
		(uuid "ba867c4c-dbd3-4921-b10b-5f23eb9a0cdf")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "TestPoint"
		(at 0 1.75 180)
		(layer "F.Fab")
		(uuid "5afe3eb6-880e-4c5b-b985-7878a9a44ea3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "TestPoint:TestPoint_Pad_D1.5mm"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4f7900af-3008-448c-b9eb-c9ff28c094b0")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1d09e0ab-fe19-4e7f-8b26-c9c57f573fa2")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" "test point"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "be6c8e50-26d6-4b8e-9724-4c92c5826e80")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_circle
		(center 0 0)
		(end 0 0.95)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "7a716a5e-0a45-4a5b-9649-b2b7c163cdcc")
	)
	(fp_circle
		(center 0 0)
		(end 1.25 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "c698d5af-26fb-4f0a-805b-f88de7ad7300")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.65 180)
		(layer "F.Fab")
		(uuid "8aa38643-12b6-4905-8920-12ff6f8ce9ea")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd circle
		(at 0 0 180)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "a6e371b0-4a45-4fd4-a097-0ff5bef6a5d7")
	)
)