(footprint "TestPoint_Pad_D1.0mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SMD pad as test Point, diameter 1.0mm")
	(tags "test point SMD pad")
	(property "Reference" "REF**"
		(at -1.68 -0.05 -90)
		(layer "F.SilkS")
		(uuid "46ae5646-35f7-491a-b343-7c0335075a30")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "TestPoint"
		(at 0 1.55 0)
		(layer "F.Fab")
		(uuid "699cd42a-1cc2-4ab6-9ced-aff0c2fb902b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cd457654-a688-414f-b6d7-0f5c2a94d388")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "40aad482-4930-4b98-8bb2-3bfe82b3fca8")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5ad61253-69c7-45c1-afca-a6ea250bead5")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" ""
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "5e446f10-0c6a-43b8-a433-8b1980fa3d89")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" ""
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "2d1af555-ed47-4aa1-a9e3-cd9098691d49")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "d789674e-dd82-4a27-a1bb-e399b0318fda")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2b968966-d8e5-4569-8f94-1494668d4c74")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr exclude_from_pos_files)
	(fp_circle
		(center 0 0)
		(end 0 0.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "788f2278-b181-49dc-b3f0-88cbdf342c8a")
	)
	(fp_circle
		(center 0 0)
		(end 1 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "0b3aca94-6ac5-4058-8386-8bc55b5d9c60")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.45 0)
		(layer "F.Fab")
		(uuid "9068d3e9-9ecb-46f9-b122-b554cf8f3942")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd circle
		(at 0 0)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c4e13ef5-c220-4ed9-89b8-169920b8eb91")
	)
)