(footprint "MountingHole_3.2mm_M3_Pad_Via"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Mounting Hole 3.2mm, M3")
	(tags "mounting hole 3.2mm m3")
	(property "Reference" "REF**"
		(at -0.66 -4.11 0)
		(layer "F.SilkS")
		(uuid "e3cbc8e7-21b6-476f-a059-028c2df0e2e2")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "MountingHole_Pad"
		(at 0 4.2 0)
		(layer "F.Fab")
		(uuid "42222ef3-b83f-41f1-8327-ca531fb17642")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "24b2a4a9-83a7-4399-9235-22913bf56a60")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b9e6b840-e3df-4ed9-b7e3-773781a7d579")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c168564a-f7c0-4207-b6ad-71039e6dbbf0")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9296674d-52b7-4c23-a72e-b2467a525d9d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_circle
		(center 0 0)
		(end 3.2 0)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill none)
		(layer "Cmts.User")
		(uuid "b1d22471-90d4-4b18-ab6b-ba07f9155d19")
	)
	(fp_circle
		(center 0 0)
		(end 3.45 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "5fd9cf30-ecdc-4eeb-9b4e-24882bd642f6")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "db27848b-e817-4d9d-8be0-1c5078c87f2c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at -2.4 0)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "a16698fe-c74d-4d00-8df6-b43df88b4fab")
	)
	(pad "1" thru_hole circle
		(at -1.697056 -1.697056)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "a903a9a9-b7e2-4867-8715-074250a8efee")
	)
	(pad "1" thru_hole circle
		(at -1.697056 1.697056)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "4dd15330-990e-4055-8b09-acfe91f89d7a")
	)
	(pad "1" thru_hole circle
		(at 0 -2.4)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "96d45c5f-4741-40de-972a-80926c1cc720")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 6.4 6.4)
		(drill 3.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "95fce717-e432-4a2a-afb5-2069ce5fb020")
	)
	(pad "1" thru_hole circle
		(at 0 2.4)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "7d5cda68-a5bd-414e-95c7-e65858a82568")
	)
	(pad "1" thru_hole circle
		(at 1.697056 -1.697056)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "fda9e0c5-fd1c-49c3-8f7f-4fc531c0636a")
	)
	(pad "1" thru_hole circle
		(at 1.697056 1.697056)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "9f41772d-4852-445d-b0de-ee214cd74d05")
	)
	(pad "1" thru_hole circle
		(at 2.4 0)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "2e5a4533-9358-462d-b7b5-c065b27fa37a")
	)
)