(footprint "CP_Elec_6.3x7.7"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SMD capacitor, aluminum electrolytic, Nichicon, 6.3x7.7mm")
	(tags "capacitor electrolytic")
	(property "Reference" "REF**"
		(at -3.74 -3.22 0)
		(layer "F.SilkS")
		(uuid "2934db21-f12b-42ec-9574-aaf84b3e946c")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "560uF/25V"
		(at 0 4.35 0)
		(layer "F.Fab")
		(uuid "d2448c18-97d6-47ac-91d2-a788dde64ea2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Capacitor_SMD:CP_Elec_6.3x7.7"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "806ebb76-a18f-46f5-a177-404671c5c33d")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c8cd4037-9392-4889-96c0-1a99aa292158")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "45b2847d-2a31-4d8c-8c88-0e9ad2bdbec1")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "fed33aa8-65bb-48fe-a3d6-e0573c987afa")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "贴片铝电解电容6.3*7.7-470UF-6.3V"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "4eba5599-34c7-4dfe-a79f-392e9adea464")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" "C5x5.8"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "65b5b9df-1920-43a6-8c16-63e4b92452b8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8e42cb80-f9de-4e83-b871-b0e91c68440d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -4.4375 -1.8475)
		(end -3.65 -1.8475)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e246c948-1d63-462b-9aae-b7f022f3fd28")
	)
	(fp_line
		(start -4.04375 -2.24125)
		(end -4.04375 -1.45375)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f6dc8079-eec2-4f9f-b257-bdb978fa2bad")
	)
	(fp_line
		(start -3.41 -2.345563)
		(end -3.41 -1.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3d5df9cd-006d-4473-8af6-cb2879bf9c41")
	)
	(fp_line
		(start -3.41 -2.345563)
		(end -2.345563 -3.41)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0d16fdf8-6431-47d8-abf5-3eb03a29f3c2")
	)
	(fp_line
		(start -3.41 2.345563)
		(end -3.41 1.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1d5cc940-6b43-49c7-b207-31ee954e05e1")
	)
	(fp_line
		(start -3.41 2.345563)
		(end -2.345563 3.41)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8030362f-c9dd-4118-9dc2-cd362526ecda")
	)
	(fp_line
		(start -2.345563 -3.41)
		(end 3.41 -3.41)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a6880573-0da9-4ab7-9003-f6afacf73525")
	)
	(fp_line
		(start -2.345563 3.41)
		(end 3.41 3.41)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "34d13377-4400-4980-93f3-ebd698625fde")
	)
	(fp_line
		(start 3.41 -3.41)
		(end 3.41 -1.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "16a2828b-8736-4ae4-9274-35424659cc4c")
	)
	(fp_line
		(start 3.41 3.41)
		(end 3.41 1.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3c4f3a76-9406-4d13-bf7c-1a26740db0c0")
	)
	(fp_line
		(start -4.7 -1.05)
		(end -4.7 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a278bbd9-597f-424f-8675-3a207e325b25")
	)
	(fp_line
		(start -4.7 1.05)
		(end -3.55 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ed1c0d1f-8543-4107-9a0d-18afc39651e0")
	)
	(fp_line
		(start -3.55 -2.4)
		(end -3.55 -1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5ba0d40c-ce55-4431-8e75-6e32cd71f4a8")
	)
	(fp_line
		(start -3.55 -2.4)
		(end -2.4 -3.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d262cc34-94b0-46fb-a8af-aaba43e06b9f")
	)
	(fp_line
		(start -3.55 -1.05)
		(end -4.7 -1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "46c3586d-3f12-401e-84df-58ae1fe16d52")
	)
	(fp_line
		(start -3.55 1.05)
		(end -3.55 2.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "58d25ed5-cad3-4f98-94b9-64725a1ba9ea")
	)
	(fp_line
		(start -3.55 2.4)
		(end -2.4 3.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5b207d40-3e17-4d25-ba24-96bbac0aec06")
	)
	(fp_line
		(start -2.4 -3.55)
		(end 3.55 -3.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "45d4f81a-e0fe-4190-beb9-420b23377ce8")
	)
	(fp_line
		(start -2.4 3.55)
		(end 3.55 3.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "65ad2d01-fc6c-4204-b8fd-8117c8099733")
	)
	(fp_line
		(start 3.55 -3.55)
		(end 3.55 -1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "636a0468-ea1a-43fc-8b49-9d7e6cc2afef")
	)
	(fp_line
		(start 3.55 -1.05)
		(end 4.7 -1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2fa2793c-0b29-4772-84d7-71a0538cb524")
	)
	(fp_line
		(start 3.55 1.05)
		(end 3.55 3.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "78b1f3a4-a802-43fc-ae05-8cb2185fe18c")
	)
	(fp_line
		(start 4.7 -1.05)
		(end 4.7 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "26cc9bf0-9403-465b-891a-1b0040c4e3f7")
	)
	(fp_line
		(start 4.7 1.05)
		(end 3.55 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fe139529-883e-4014-8b4b-85ddfc0f10a4")
	)
	(fp_line
		(start -3.3 -2.3)
		(end -3.3 2.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "635ec8f9-86c8-4126-b5d0-9a28ebcbf21d")
	)
	(fp_line
		(start -3.3 -2.3)
		(end -2.3 -3.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b7114bcc-9cf8-4bda-9faa-13eb11289c92")
	)
	(fp_line
		(start -3.3 2.3)
		(end -2.3 3.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d48a8607-b618-429b-bad7-65609ae0f7b5")
	)
	(fp_line
		(start -2.704838 -1.33)
		(end -2.074838 -1.33)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5c2c0a0c-c8f7-4b1f-b886-0876c3f1f23c")
	)
	(fp_line
		(start -2.389838 -1.645)
		(end -2.389838 -1.015)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2f30ffd0-df87-44b3-b1fc-a26d6d76687c")
	)
	(fp_line
		(start -2.3 -3.3)
		(end 3.3 -3.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1fbea799-1e93-4fbb-b921-c5abee642d9a")
	)
	(fp_line
		(start -2.3 3.3)
		(end 3.3 3.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c0bae3cf-0a2c-4443-9940-24c06806bece")
	)
	(fp_line
		(start 3.3 -3.3)
		(end 3.3 3.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "135cd7ca-f769-4ba5-8314-1693fe7c100b")
	)
	(fp_circle
		(center 0 0)
		(end 3.15 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "c43071b9-9b68-414d-8dd0-0703a3a769c5")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "e3e6dc8f-0ea3-4f00-a7c3-752421b1a462")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.7 0)
		(size 3.5 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.15625)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "17cfff57-eaa6-4946-acf3-583f60742194")
	)
	(pad "2" smd roundrect
		(at 2.7 0)
		(size 3.5 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.15625)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "a0e8c329-c57a-4864-bcb3-8e7024d1a60c")
	)
	(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x7.7.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)