(footprint "TSOT-23-6"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "TSOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "TSOT TO_SOT_SMD")
	(property "Reference" "REF**"
		(at 0.67 2.265 180)
		(layer "F.SilkS")
		(uuid "e9f8fdc7-ea76-4250-8992-503876140152")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "SY8253ADC"
		(at 0 2.4 180)
		(layer "F.Fab")
		(uuid "9cee640f-f805-4a56-8627-52b8c7c31807")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "31c263b3-582a-4da5-8b43-c192fc79e1f6")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" "https://atta.szlcsc.com/upload/public/pdf/source/20180625/C93736_E75EC6FD4320D65590D2D5BF0D8B8959.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e185be70-6215-485f-b908-e05fd4e98757")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5dfe8500-a353-4a18-92c7-04d43f4f1e09")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" "https://item.szlcsc.com/94934.html"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "b871c6f8-e5fa-4cda-8b2e-ce8fcc6b6d57")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "Buck IC-SY8253ADC-TSOT-23-6"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "eee01db3-dd40-4b88-a9a0-10e13f041169")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "d8d05050-a1b2-4cb7-a4d3-1c7ba8be9f17")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f7c7ef8e-f246-45b7-8e8e-0827d58162e2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0 -1.56)
		(end -0.5 -1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2e9f84bf-376a-4c80-8e7d-e724ff52a307")
	)
	(fp_line
		(start 0 -1.56)
		(end 0.8 -1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "59d16377-7d70-4890-841d-ad0ca2d85606")
	)
	(fp_line
		(start 0 1.56)
		(end -0.8 1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c45aaebb-dfbb-4cde-8845-1d9a887f5b6c")
	)
	(fp_line
		(start 0 1.56)
		(end 0.8 1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c9906823-56f3-48b2-bc8d-8835030f2978")
	)
	(fp_circle
		(center -1.12 -1.56)
		(end -0.92 -1.56)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "b814c3cd-bb33-42fb-8479-773c7ffb2e54")
	)
	(fp_line
		(start -2.05 -1.7)
		(end -2.05 1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6ecf0863-a387-4c5f-a59e-436a6903b32f")
	)
	(fp_line
		(start -2.05 1.7)
		(end 2.05 1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "60b89d66-1098-463e-b5e8-9caaa24dbcf2")
	)
	(fp_line
		(start 2.05 -1.7)
		(end -2.05 -1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "86bf89fc-84ae-4d7f-8912-9ef695e2e4de")
	)
	(fp_line
		(start 2.05 1.7)
		(end 2.05 -1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1f2d131f-460b-4877-b398-da68305ef150")
	)
	(fp_line
		(start -0.8 -1.05)
		(end -0.4 -1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "32118361-b4b3-49c6-a08d-b0f93a98afdb")
	)
	(fp_line
		(start -0.8 1.45)
		(end -0.8 -1.05)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b4e7c3fa-61cf-4bd0-8831-efbaebbdb106")
	)
	(fp_line
		(start -0.4 -1.45)
		(end 0.8 -1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "912de1e2-5c68-46f7-8e40-64726627d932")
	)
	(fp_line
		(start 0.8 -1.45)
		(end 0.8 1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a9a91808-e048-4228-93ed-25499c5eda0c")
	)
	(fp_line
		(start 0.8 1.45)
		(end -0.8 1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "05c7f7a6-4786-4f57-b519-158ade2441e0")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "9ea2189f-e942-48c5-ab54-dc7b52ccdb34")
		(effects
			(font
				(size 0.4 0.4)
				(thickness 0.06)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.1375 -0.95)
		(size 1.325 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "2ce5d092-655b-4deb-8d33-8a77bd34f5eb")
	)
	(pad "2" smd roundrect
		(at -1.1375 0)
		(size 1.325 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "888153dc-20ce-4266-88cf-6700b8d13210")
	)
	(pad "3" smd roundrect
		(at -1.1375 0.95)
		(size 1.325 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "98d985ca-e083-4351-a44d-d6a73201d733")
	)
	(pad "4" smd roundrect
		(at 1.1375 0.95)
		(size 1.325 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "1e7dc00d-777a-4e4f-be59-c42ec1087ead")
	)
	(pad "5" smd roundrect
		(at 1.1375 0)
		(size 1.325 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "7f4769e0-adfa-40b1-96c9-0ddefdb2236e")
	)
	(pad "6" smd roundrect
		(at 1.1375 -0.95)
		(size 1.325 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "a316af96-6624-4f6c-8cc4-cf9a1469f3c6")
	)
	(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-6.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)