(footprint "USB3_A_Molex_48406-0001_Horizontal_Stacked"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "USB 3.0, type A, right angle, stacked (https://www.molex.com/content/dam/molex/molex-dot-com/products/automated/en-us/salesdrawingpdf/484/48406/484060001_sd.pdf)")
	(tags "USB 3.0 type A right angle stacked dual")
	(property "Reference" "REF**"
		(at 9.830001 -7.08 0)
		(layer "F.SilkS")
		(uuid "b0f81163-733d-454a-be48-08c0386e6329")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "USB3_A_Stacked"
		(at 3.5 13 0)
		(layer "F.Fab")
		(uuid "7faffd54-2b2a-4102-9eea-e37992a3c027")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_USB:USB3_A_Molex_48406-0001_Horizontal_Stacked"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "80b01f1b-e489-4cf3-b432-a8e52ee947dc")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8f4fe8e5-8273-46b3-9e17-daa9961d0567")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "29bc7626-e30d-406c-a00b-bb864c36b8be")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" "https://item.szlcsc.com/3132965.html"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b5e9207b-c71a-4535-bdcf-69ebc56d82be")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "双层USB3.0 A母座_USB-303WSD-BRY"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "94b18128-d484-4023-8dba-552cda0d9276")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "c7f3347d-1d76-4ee2-abf2-d165702a6b76")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5fe300ff-44c8-4558-8ffd-59319409c9ce")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -4.5 -0.5)
		(end -4.5 0.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2b9f7b02-2503-444e-bab0-f4a270eb85cd")
	)
	(fp_line
		(start -4.5 0.5)
		(end -4 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "63df68cc-24dc-46b3-9048-7dc7ea23d7e8")
	)
	(fp_line
		(start -4 0)
		(end -4.5 -0.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "eafa9733-c2ab-4126-94cd-7b31c4696483")
	)
	(fp_line
		(start -3.46 -6.08)
		(end -3.46 -5.78)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5ede3dde-9720-48e9-af95-e2428b4ff4b5")
	)
	(fp_line
		(start -3.46 -6.08)
		(end 10.46 -6.08)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ad726db0-8833-444c-b8f4-923b0aee87ca")
	)
	(fp_line
		(start -3.46 -0.1)
		(end -3.46 -1.58)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5a4266ad-f909-4a3b-a1c0-cb54436b5e84")
	)
	(fp_line
		(start -3.46 6.8)
		(end -3.46 4.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b7b2acc6-5d73-4eb5-90b1-f80ffd951ff3")
	)
	(fp_line
		(start 10.46 -6.08)
		(end 10.46 -5.78)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7827a016-7e26-4408-8458-b2625923b29b")
	)
	(fp_line
		(start 10.46 -0.1)
		(end 10.46 -1.58)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e5ed9343-ddb5-4b1a-aa50-0b41e84e1c6f")
	)
	(fp_line
		(start 10.46 6.8)
		(end 10.46 4.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "96968224-5fa8-448d-8c1a-1fea698954aa")
	)
	(fp_line
		(start -4.25 10.44)
		(end -3.9 10.44)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4c6affd6-64df-4908-8a6e-4e3b0afbcca5")
	)
	(fp_line
		(start -4.25 11.94)
		(end -4.25 10.44)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3ed61ce0-b6eb-4cdf-8053-a9f4d631c682")
	)
	(fp_line
		(start -3.9 -6.52)
		(end 10.9 -6.52)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ca69eada-8aa4-48d3-b31f-0bbe494157e3")
	)
	(fp_line
		(start -3.9 -5.77)
		(end -3.9 -6.52)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f7e00d28-0ced-4478-b857-aba31a806a75")
	)
	(fp_line
		(start -3.9 -0.09)
		(end -3.9 -1.59)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "bfc22beb-f22f-4ae1-ae74-dac7ab4898d9")
	)
	(fp_line
		(start -3.9 10.44)
		(end -3.9 4.09)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fc1c7f44-315f-4b5e-be2f-bac14cbe28aa")
	)
	(fp_line
		(start -3.9 11.94)
		(end -4.25 11.94)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7cd5f22a-ff5f-4805-a0b5-9b8a64bbc3a3")
	)
	(fp_line
		(start -3.9 11.94)
		(end 10.9 11.94)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "00875e6e-2a28-4c5e-9fa1-a9c216d2e237")
	)
	(fp_line
		(start 10.9 -6.52)
		(end 10.9 -5.77)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d8ef147b-aa6b-4dbe-9e07-d486e3da55a5")
	)
	(fp_line
		(start 10.9 -1.59)
		(end 10.9 -0.09)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9958fb69-6e27-4628-b190-408d8b5d0ee2")
	)
	(fp_line
		(start 10.9 4.09)
		(end 10.9 10.44)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7fde6204-b5a6-4619-8efb-4314611d0014")
	)
	(fp_line
		(start 10.9 11.94)
		(end 11.25 11.94)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "555cabef-4bfb-4273-be05-1420309eedea")
	)
	(fp_line
		(start 11.25 10.44)
		(end 10.9 10.44)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "27c7be3e-92b5-462a-b1c0-b01b5a3b4dc9")
	)
	(fp_line
		(start 11.25 11.94)
		(end 11.25 10.44)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5f24388f-af90-4a15-bf3b-fdad67734761")
	)
	(fp_arc
		(start -3.9 -1.59)
		(mid -5.32 -3.68)
		(end -3.9 -5.77)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d15db3bd-a75b-46e6-a37c-4419293584fa")
	)
	(fp_arc
		(start -3.9 4.09)
		(mid -5.32 2)
		(end -3.9 -0.09)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7da933ca-d70e-45ed-987b-024384144c29")
	)
	(fp_arc
		(start 10.9 -5.77)
		(mid 12.320002 -3.68)
		(end 10.9 -1.59)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2f63af1a-0585-4aae-9c7b-56133c56ee03")
	)
	(fp_arc
		(start 10.9 -0.09)
		(mid 12.320002 2)
		(end 10.9 4.09)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c8ef7268-0167-4988-8105-4eb3100abb4a")
	)
	(fp_line
		(start -3.75 10.94)
		(end -3.4 10.94)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "7207722b-f4f6-4a9d-a6ae-7fb3fdd5ebee")
	)
	(fp_line
		(start -3.75 11.44)
		(end -3.75 10.94)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "ac2fdc15-363a-44a8-bcef-0e296dc7db17")
	)
	(fp_line
		(start -3.4 -6.02)
		(end 10.4 -6.02)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "871cd6a6-29ac-4715-ac59-48d269dc28f2")
	)
	(fp_line
		(start -3.4 0.5)
		(end -2.9 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ac6bbc78-f85b-4dda-9a4b-7e678206db28")
	)
	(fp_line
		(start -3.4 10.94)
		(end -3.4 -6.02)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b2a097c6-c958-45be-a65a-be53f0a0f3dd")
	)
	(fp_line
		(start -2.9 0)
		(end -3.4 -0.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "02e83aba-55ac-4987-a121-475dcba04a8b")
	)
	(fp_line
		(start 10.4 -6.02)
		(end 10.4 10.94)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "88ee4900-021e-4f16-8bca-7503484e7309")
	)
	(fp_line
		(start 10.75 10.94)
		(end 10.4 10.94)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "85941ce9-ab55-40b9-95f1-018be9cf80e6")
	)
	(fp_line
		(start 10.75 11.44)
		(end -3.75 11.44)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c97b68a9-351b-4bd5-a6c2-b6282ad55e8f")
	)
	(fp_line
		(start 10.75 11.44)
		(end 10.75 10.94)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "9669f647-6ba3-49e5-a5c5-4e58b6f59eac")
	)
	(fp_text user "${REFERENCE}"
		(at 3.5 5 0)
		(layer "F.Fab")
		(uuid "64a481da-9825-47cb-a2a4-7dd8a81e4ca2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "9f907e0d-bd87-43bb-81af-088fe491a1f3")
	)
	(pad "2" thru_hole circle
		(at 2.5 0)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "84573699-6d93-4371-9d8d-0c637498809a")
	)
	(pad "3" thru_hole circle
		(at 4.5 0)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "2a4afb34-92df-446c-9fa8-77fb40770107")
	)
	(pad "4" thru_hole circle
		(at 7 0)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "f49f78d3-c9e0-40e5-8130-87f4b9e670b9")
	)
	(pad "5" thru_hole circle
		(at 7.5 -1.5)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c0c0b60e-c5ac-4a65-abf7-f5b60251b144")
	)
	(pad "6" thru_hole circle
		(at 5.5 -1.5)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "13ba18b8-c04c-4838-8582-f63d54b12902")
	)
	(pad "7" thru_hole circle
		(at 3.5 -1.5)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "91b55312-eac5-4264-88b9-e8bea2212085")
	)
	(pad "8" thru_hole circle
		(at 1.5 -1.5)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "0b97f44c-4f41-41e8-8342-2de14ba33769")
	)
	(pad "9" thru_hole circle
		(at -0.5 -1.5)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c1a33fcb-b3d1-458f-9dc6-c42bd6be4519")
	)
	(pad "10" thru_hole circle
		(at 0 -3.2)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "d0094b28-27c2-4ff6-9351-15c2f679a0fd")
	)
	(pad "11" thru_hole circle
		(at 2.5 -3.2)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "1d7dd444-6e4f-40d6-8ef8-f7d37e96e4db")
	)
	(pad "12" thru_hole circle
		(at 4.5 -3.2)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "45214137-fa4b-4a51-8a37-3de2686b23ca")
	)
	(pad "13" thru_hole circle
		(at 7 -3.2)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "6f9a8f1f-4076-4bea-a916-777aa15f8b86")
	)
	(pad "14" thru_hole circle
		(at 7.5 -4.7)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "0f435e52-bc57-4677-8d96-e683416d6282")
	)
	(pad "15" thru_hole circle
		(at 5.5 -4.7)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "fe292670-6a90-4d53-9a18-20359fdb75e7")
	)
	(pad "16" thru_hole circle
		(at 3.5 -4.7)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "2ae956ba-650f-41d6-8b92-9db9b2349e77")
	)
	(pad "17" thru_hole circle
		(at 1.5 -4.7)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "92aca5d5-7c2d-4be5-85f1-a9e3392ea9a0")
	)
	(pad "18" thru_hole circle
		(at -0.5 -4.7)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "b40d4178-1eb3-4480-aeba-7c785d78e78a")
	)
	(pad "19" thru_hole circle
		(at -3.07 -3.68)
		(size 3.5 3.5)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "a41c0d63-7d2b-4ba7-928b-8cc773a29141")
	)
	(pad "19" thru_hole circle
		(at -3.07 2)
		(size 3.5 3.5)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "3ab8c6a2-1f50-458e-8856-451d21cf65b4")
	)
	(pad "19" thru_hole circle
		(at 10.07 -3.68)
		(size 3.5 3.5)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "0c00bc86-e3f8-4607-a590-cfd8dc8c6440")
	)
	(pad "19" thru_hole circle
		(at 10.07 2)
		(size 3.5 3.5)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "dccfa4c9-00cb-447d-804e-0e4652c32314")
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_USB.3dshapes/USB3_A_Molex_48406-0001_Horizontal_Stacked.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "D:/项目/2023样品项目/LattePanda Mu/LIB_48406-0003/48406-0003/3D/48406-0003.stp"
		(offset
			(xyz -3.1 -11.2 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 90 0)
		)
	)
)