(footprint "MountingHole_2.7mm_M2_Pad_TopOnly"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Mounting Hole 3.2mm, M3, DIN965")
	(tags "mounting hole 3.2mm m3 din965")
	(property "Reference" "REF**"
		(at 0 -3.8 0)
		(layer "F.SilkS")
		(uuid "dc69ae86-aae2-4d54-9047-c57d5be325b1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "MountingHole_2.7mm_M2_Pad_TopOnly"
		(at 0 3.8 0)
		(layer "F.Fab")
		(uuid "62947aba-e4e3-408d-8e60-75ee1d660412")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3dde2ad6-4fb3-4675-87c0-eac78a05c769")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "92689061-b603-4892-aabe-39dcbec3b067")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b2ff81f7-833f-409d-a483-01e158bb9313")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_circle
		(center 0 0)
		(end 2.8 0)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill none)
		(layer "Cmts.User")
		(uuid "84810a35-635b-4b9d-9eff-6229dc6d66f0")
	)
	(fp_circle
		(center 0 0)
		(end 3.05 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "1f15379e-2261-4849-a2c4-e47e8855aaad")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "7260bb4d-2274-4eda-9a37-a3068a7d99a9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.9 2.9)
		(drill 2.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d001223d-8e09-4af5-95d2-32779f81fef7")
	)
	(pad "1" connect circle
		(at 0 0)
		(size 4 4)
		(layers "F.Cu" "F.Mask")
		(uuid "42864e21-e8c1-4fac-9c58-c175fdb95d11")
	)
)