(footprint "SOT-23"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "SOT TO_SOT_SMD")
	(property "Reference" "REF**"
		(at 1.405 -1.37 90)
		(layer "F.SilkS")
		(uuid "d474fbd2-68ad-4957-ae30-40e5e0d59ae3")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "2SK3018"
		(at 0 2.4 0)
		(layer "F.Fab")
		(uuid "d151f57f-9ce7-4cb0-8fdf-e4bd5984db39")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ae5f3365-d88e-4882-9591-56be4ac89581")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NDS7002A-D.PDF"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f8d61001-13ea-40dc-aede-87199cbc5d29")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "18dc9b1c-6ab8-4112-8e66-d65ac7b10e25")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" "https://item.szlcsc.com/774253.html"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "addd36b4-943f-448a-940f-7b1fc089e96f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "NMOS_2SK3018_SOT-23"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "09fa3ea3-39dc-453c-8ee0-a9626efa9fd2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "b824efb9-4961-4457-95f6-237fee67c9a4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0b744eb5-6028-41f5-a7e2-c8ddbc3afdce")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0 -1.56)
		(end -1.675 -1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3c07666f-4d28-4a96-9c7c-fe3b6a820601")
	)
	(fp_line
		(start 0 -1.56)
		(end 0.65 -1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "de915487-fb58-4c4e-8ff4-90df096e559e")
	)
	(fp_line
		(start 0 1.56)
		(end -0.65 1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "49a4ed08-5887-449a-9818-b7ec2ff4ad23")
	)
	(fp_line
		(start 0 1.56)
		(end 0.65 1.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9e4eaf69-bcb0-4c7b-83a4-39e0f50d60d1")
	)
	(fp_line
		(start -1.92 -1.7)
		(end -1.92 1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "914b4c54-4dbc-49f1-a5cd-a6a80b691b1e")
	)
	(fp_line
		(start -1.92 1.7)
		(end 1.92 1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fb352763-c058-459f-b445-24482fe3fbc7")
	)
	(fp_line
		(start 1.92 -1.7)
		(end -1.92 -1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "0f6f4b1f-1f51-4547-9b69-c8e5ad8671a8")
	)
	(fp_line
		(start 1.92 1.7)
		(end 1.92 -1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a29da5f1-e516-483f-899a-9cb1d65e2a04")
	)
	(fp_line
		(start -0.65 -1.125)
		(end -0.325 -1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "67bf6f92-4c3f-4278-848c-a087236b5fea")
	)
	(fp_line
		(start -0.65 1.45)
		(end -0.65 -1.125)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ed951f2a-1765-4b75-b824-e60716dae179")
	)
	(fp_line
		(start -0.325 -1.45)
		(end 0.65 -1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c90f02cb-4915-4b6d-bb2e-c587e34b0623")
	)
	(fp_line
		(start 0.65 -1.45)
		(end 0.65 1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "783980e2-9ef3-4045-b80e-6d7c1214c85f")
	)
	(fp_line
		(start 0.65 1.45)
		(end -0.65 1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5a47bf18-aab5-4fef-9466-392ece64b4b9")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "0faec78b-c239-4d97-8498-250769af05cc")
		(effects
			(font
				(size 0.32 0.32)
				(thickness 0.05)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.9375 -0.95)
		(size 1.475 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c4efc515-0150-4f69-a2e7-7112817676f8")
	)
	(pad "2" smd roundrect
		(at -0.9375 0.95)
		(size 1.475 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "91fcdcda-988d-471e-95bd-00b7727e9d8a")
	)
	(pad "3" smd roundrect
		(at 0.9375 0)
		(size 1.475 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "902f14dd-88c5-41c2-a122-50a8ab517f99")
	)
	(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)