(footprint "Fiducial_0.5mm_Mask1mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
	(tags "fiducial")
	(property "Reference" "REF**"
		(at 0.02 1.41 0)
		(layer "F.SilkS")
		(uuid "c0bd6586-f148-40c9-8f4c-ba1edd9f2526")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Fiducial"
		(at 0 1.5 0)
		(layer "F.Fab")
		(uuid "4ad77c72-c642-4c0e-a976-a846e298d8d3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Fiducial:Fiducial_0.5mm_Mask1mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "195223ac-8f2b-4768-a77b-60b5336189f7")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "290c9152-890e-4237-8b3f-f1b26fd8611f")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f403f6cf-3313-4169-9c1f-48e41c096e14")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c2dc16fa-57c3-443a-860a-6e796dc0c82b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd exclude_from_bom)
	(fp_circle
		(center 0 0)
		(end 0.75 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "f763fb54-caaf-4b97-8d9a-79d1dc61162e")
	)
	(fp_circle
		(center 0 0)
		(end 0.5 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "2424f371-da68-4a3c-999f-f2fb7b167356")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "bd528590-6970-4e83-8c76-e19c5a1b64c9")
		(effects
			(font
				(size 0.2 0.2)
				(thickness 0.04)
			)
		)
	)
	(pad "" smd circle
		(at 0 0)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.25)
		(clearance 0.25)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "4fdc8bb0-1448-470c-ae10-07e153cb45f4")
	)
)