(footprint "L_Sunlord_SWPA4020S"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Inductor, Sunlord, SWPA4020S, 4.0x4.0x2.0mm, https://www.sunlordinc.com/UploadFiles/PDF_Cat/20120704094224784.pdf")
	(tags "Inductor swpa")
	(property "Reference" "REF**"
		(at 0.02 -2.85 0)
		(layer "F.SilkS")
		(uuid "4eafe148-c370-405d-bb49-517c4b3d1ace")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "2.2uH/4.3A"
		(at 0 3 180)
		(layer "F.Fab")
		(uuid "e126504f-9697-48e0-8e7c-bd659887f9e1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Inductor_SMD:L_Sunlord_SWPA4020S"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "098ad139-2091-468f-b46a-e570939d8158")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "788b57a9-fdac-4999-ad7f-9161fd5c92e3")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d4aec6e0-6a7d-43c2-8fe1-5bfa1cb6a224")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "e70e9971-4bc9-414b-9a89-cecfb4ebdacc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "贴片屏蔽电感2.2uH_4.0*4.0*2.0_4.3A"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "524d7f24-04f8-4387-9d1f-56d57d0c253e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "70b174c6-16f6-4802-a956-2e9344b2d7c5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2d4217a4-e5a3-414e-ba31-edf878e9507c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.26 -2.26)
		(end -2.26 -2.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5e2b790f-f542-480e-b92a-5af28b08212f")
	)
	(fp_line
		(start -2.26 -2.26)
		(end 2.26 -2.26)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5444e90d-d20a-4c2b-a1c2-1c6a5afd6ece")
	)
	(fp_line
		(start -2.26 2.26)
		(end -2.26 2.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "35f3ff0d-ce85-4330-a757-85c25d62a697")
	)
	(fp_line
		(start -2.26 2.26)
		(end 2.26 2.26)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9356db6c-250f-4f84-bf6d-42ee334ef5f1")
	)
	(fp_line
		(start 2.26 -2.26)
		(end 2.26 -2.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5e52a685-26fe-49b7-8f24-733ee1683029")
	)
	(fp_line
		(start 2.26 2.26)
		(end 2.26 2.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "91fada65-fde9-4beb-8971-bd5893ead549")
	)
	(fp_line
		(start -2.3 -2.25)
		(end -2.3 2.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7d941746-9a31-441a-837d-66cc16c53574")
	)
	(fp_line
		(start -2.3 2.25)
		(end 2.3 2.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "871eb58c-6e75-4e80-958b-8796b5c32bf9")
	)
	(fp_line
		(start 2.3 -2.25)
		(end -2.3 -2.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b7fa9017-b552-400d-823f-e99207e093f6")
	)
	(fp_line
		(start 2.3 2.25)
		(end 2.3 -2.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "0ee5a722-b62e-4b7c-8462-c5c7ac8bdf2b")
	)
	(fp_line
		(start -2 -2)
		(end -2 2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "761dff26-fb7a-41f4-a128-c4e566975ca1")
	)
	(fp_line
		(start -2 2)
		(end 2 2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2386cd48-c5fe-4dcc-b182-f0b0e87f2a24")
	)
	(fp_line
		(start 2 -2)
		(end -2 -2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4d469b53-6402-4d86-b90d-ff7a69e86704")
	)
	(fp_line
		(start 2 2)
		(end 2 -2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8d760906-d0c8-4fbc-861d-78e530262561")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "d558b859-ebdb-4bd7-950f-f02a00220525")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(pad "1" smd rect
		(at -1.5 0)
		(size 1.1 3.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "b1f8773e-bac5-4c5d-aed0-d4847dd7a655")
	)
	(pad "2" smd rect
		(at 1.5 0)
		(size 1.1 3.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c1a65f10-5a07-41fc-8f95-b7cfd81bad5c")
	)
	(model "${KICAD7_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Sunlord_SWPA4020S.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)