(footprint "Crystal_SMD_3225-4Pin_3.2x2.5mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
	(tags "SMD SMT crystal")
	(property "Reference" "REF**"
		(at 0.019739 2.335 -90)
		(layer "F.SilkS")
		(uuid "e010f427-0a35-4734-8a9f-4e1ad0f25e75")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "25MHz"
		(at 0 2.45 180)
		(layer "F.Fab")
		(uuid "f5cbb883-e596-4a6a-ab8b-ac5cdacb8c93")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bd8ab35b-93da-48d4-a8c5-a824bb9923f0")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d616a3b8-e80b-45ea-813f-fec2ed432e30")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f50f3b80-6850-4501-8488-60af6ddbc59e")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" ""
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "ea1e89dd-35e6-4199-98d6-5d6f3ffab6e3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "贴片晶振-4脚无源-25M-20ppm-3.2*2.5(3225)"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "7150b2ab-ada6-424b-9ba0-28df6cdfe7f7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "41dee8f9-0b96-4c7b-93d7-ee1cf9b48eb3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d00ef8bd-b9f9-4c32-8497-fcc6d14a4e43")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2 -1.65)
		(end -2 1.65)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c293b2f3-c832-43c9-808c-4d3faebfd16c")
	)
	(fp_line
		(start -2 0)
		(end 0 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e4ee268e-7808-4340-8e77-58818ea4fb37")
	)
	(fp_line
		(start -2 1.65)
		(end 2 1.65)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f501a31b-8b9a-42af-84c6-d9bab8de81ab")
	)
	(fp_line
		(start 0 0.01)
		(end 0 1.65)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a0771b79-a00e-4273-8209-5e8d7b769bf4")
	)
	(fp_line
		(start 2 -1.65)
		(end -2 -1.65)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2851504d-5d96-4638-b9ef-1d4ad70cb41f")
	)
	(fp_line
		(start 2 1.65)
		(end 2 -1.65)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dd3534f0-2b69-407c-838e-a53391d30e85")
	)
	(fp_line
		(start -2.1 -1.7)
		(end -2.1 1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fcffc884-d2d4-4bf5-a0a9-479ecb71e72b")
	)
	(fp_line
		(start -2.1 1.7)
		(end 2.1 1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b7c4c11e-82ac-461b-ac6c-3a3de3eb977c")
	)
	(fp_line
		(start 2.1 -1.7)
		(end -2.1 -1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ae876e6e-156f-4a84-8e0e-f553ea153141")
	)
	(fp_line
		(start 2.1 1.7)
		(end 2.1 -1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "481ea040-99c2-41fe-8d92-243b04f6e546")
	)
	(fp_line
		(start -1.6 -1.25)
		(end -1.6 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fba15d05-63f8-4e33-8628-d777445b671f")
	)
	(fp_line
		(start -1.6 0.25)
		(end -0.6 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6c47660d-9c55-4ca1-9871-a957dccb7862")
	)
	(fp_line
		(start -1.6 1.25)
		(end 1.6 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "21b95ad4-3029-4c7b-a4bf-26975ec97a2d")
	)
	(fp_line
		(start 1.6 -1.25)
		(end -1.6 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3c89defa-579c-4b7b-8461-5581c8bb9c9c")
	)
	(fp_line
		(start 1.6 1.25)
		(end 1.6 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5e6c5115-55c7-40b4-a0e1-191d4460cd74")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "2f9ef7dd-79fb-436e-808f-9f3b6c998bcc")
		(effects
			(font
				(size 0.7 0.7)
				(thickness 0.105)
			)
		)
	)
	(pad "1" smd rect
		(at -1.1 0.85)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "3952ecf9-0af2-4432-957c-00e17f7bbaf2")
	)
	(pad "2" smd rect
		(at 1.1 0.85)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "9ce0fec3-569b-4c2a-bb76-1a156d588ea6")
	)
	(pad "3" smd rect
		(at 1.1 -0.85)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "37574a02-3ff9-409e-9b5b-def9255b3b15")
	)
	(pad "4" smd rect
		(at -1.1 -0.85)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c99736f0-604a-4ba4-9f5d-4f59cb7b4011")
	)
	(model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)