(footprint "MOSFET_PDFN8_3.3x3.3"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr " DFN 3x3  EP")
	(tags "MOSFET (N-Channel)")
	(property "Reference" "REF**"
		(at 0.215 -2.61 90)
		(layer "F.SilkS")
		(uuid "fa43152a-485d-4203-9854-d03542b3b321")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "NCE30P28Q"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "cb72c28f-d97c-4e19-bf05-e4003937a526")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.254)
			)
		)
	)
	(property "Footprint" "Package_DFN_QFN:MOSFET_PDFN8_3.3x3.3"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "72f9a81b-f8c4-46d6-baa8-b3a551402eda")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1187c4be-753c-4a41-915c-64b453a19eb6")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "488d4d81-e560-4f46-90fb-7ff69773c180")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "DF_Comment" "PMOS管NCE30P28Q-DFN3.3X3.3-8L"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "324a006e-cb8f-486a-8423-17beb5711823")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4a6918ae-6a70-4acc-bb88-78e62a355ac2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.975 2.1)
		(end -0.975 2.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d318dc44-0406-4630-850c-3f7a20985c31")
	)
	(fp_line
		(start -0.975 2.2)
		(end -0.975 2.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dab170aa-c0ab-4919-84a3-ea8b9d75b10a")
	)
	(fp_arc
		(start -0.975 2.1)
		(mid -0.925 2.15)
		(end -0.975 2.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "49e3fef4-b263-451d-a4fd-6cf5d0c63770")
	)
	(fp_arc
		(start -0.975 2.2)
		(mid -1.025 2.15)
		(end -0.975 2.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "64e7fbe6-6512-49e7-9d60-68caa945f59d")
	)
	(fp_line
		(start -2.605 -2.65)
		(end 2.605 -2.65)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f0736374-0b8d-4d4f-8678-549745814a90")
	)
	(fp_line
		(start -2.605 2.65)
		(end -2.605 -2.65)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e77e687a-1069-4afc-a37e-52de71b19b1d")
	)
	(fp_line
		(start 2.605 -2.65)
		(end 2.605 2.65)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "dd267b32-533d-4d0e-b821-e0836e5f9e6b")
	)
	(fp_line
		(start 2.605 2.65)
		(end -2.605 2.65)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c28f5e53-a0cd-4bbd-9cd6-b1b0721d8980")
	)
	(fp_line
		(start -1.5 -1.5)
		(end 1.5 -1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4351a0ad-1059-4c98-8363-502b0fc94aa5")
	)
	(fp_line
		(start -1.5 1.5)
		(end -1.5 -1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c84734b3-65fa-4e5d-8fc1-3fc96d5ec5d8")
	)
	(fp_line
		(start 1.5 -1.5)
		(end 1.5 1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d16baf85-053e-4d09-8838-a1245c485226")
	)
	(fp_line
		(start 1.5 1.5)
		(end -1.5 1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b00aac72-bacf-4b77-941f-bf847b8da4de")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "a6febbaf-d8a0-42d8-96f2-32d00091b7ad")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.254)
			)
		)
	)
	(pad "1" smd rect
		(at -0.975 1.4)
		(size 0.35 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "4fc70600-c15d-4369-8221-11e14055e2c4")
	)
	(pad "2" smd rect
		(at -0.325 1.4)
		(size 0.35 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "1d78c62b-eb9d-4618-ba47-38f80da76a0f")
	)
	(pad "3" smd rect
		(at 0.325 1.4)
		(size 0.35 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c7ad9461-ea6c-4630-a540-82bfc5f97b33")
	)
	(pad "4" smd rect
		(at 0.975 1.4)
		(size 0.35 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "f5fb1db3-f9e2-4e26-9e6b-de55049e402f")
	)
	(pad "5" smd rect
		(at 0.975 -1.5 90)
		(size 0.3 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "0d87570b-5556-4244-936d-f5f08903b206")
	)
	(pad "6" smd rect
		(at 0.325 -1.5 90)
		(size 0.3 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "19031978-8320-4fc5-9215-c358f901447c")
	)
	(pad "7" smd rect
		(at -0.325 -1.5 90)
		(size 0.3 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "d551fae9-077e-4877-9793-ff34a8d3bb50")
	)
	(pad "8" smd rect
		(at -0.975 -1.5 90)
		(size 0.3 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "a7be249e-b917-4090-aeb9-9cd74441acb0")
	)
	(pad "9" smd rect
		(at 0 -0.36 90)
		(size 1.98 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "017a379e-6fae-46b5-ae53-427adf1da51c")
	)
	(pad "10" smd rect
		(at 1.415 0)
		(size 0.38 0.43)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c0c26e6e-3086-4439-b1dd-5de345a0844b")
	)
	(pad "11" smd rect
		(at -1.415 0)
		(size 0.38 0.43)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c15bb8de-31cf-4b72-b749-010d06825370")
	)
	(model "AON7262E.stp"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "D:/项目/2023样品项目/LattePanda Mu/AON7262E/3D/AON7262E.stp"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)