(footprint "Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "U-DFN2510-10 package used by Diodes Incorporated (https://www.diodes.com/assets/Package-Files/U-DFN2510-10-Type-CJ.pdf)")
	(tags "UDFN-10 U-DFN2510-10 Diodes")
	(property "Reference" "REF**"
		(at -1.2925 0.029999 90)
		(layer "F.SilkS")
		(uuid "5857c26f-f917-4cd8-8e6c-a45220326a39")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "ULC0524P"
		(at 0 2.54 180)
		(layer "F.Fab")
		(uuid "f5de163a-4197-461c-83fb-9c431eb24234")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f8398e8b-7a75-47fa-8101-f63a7246531d")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" "https://www.diodes.com/assets/Datasheets/D3V3XA4B10LP.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "051b7b51-6a50-4822-aeec-7a2768a2420f")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "67a197f9-1409-4a23-8c7e-a3a2f1a8a473")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Buy_Link" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "de56525c-9bfc-4007-bec8-a6c74fcc9208")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "DF_Comment" "ESD静电保护IC-BV-ULC0524P-DFN2510-10L"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "7d174aa5-9af8-474d-9567-0988f49b16df")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "SCH_Show_Footprint" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "62b534c2-51a7-49cb-aaa3-f39434bf7570")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c4de94ba-bf71-4387-b50b-216a30888e2c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0.5 -1.35)
		(end 0 -1.35)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e85cf316-5a44-42cf-a62a-830afcc0d055")
	)
	(fp_line
		(start 0.5 1.35)
		(end -0.5 1.35)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "df458f69-bf00-458f-b863-01905445ea3e")
	)
	(fp_line
		(start -0.95 -1.5)
		(end 0.95 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9215a03f-f85b-497a-93b9-f5136fc38c6f")
	)
	(fp_line
		(start -0.95 1.5)
		(end -0.95 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "cabbd72f-2ecb-4147-85f4-2401cf49aeed")
	)
	(fp_line
		(start 0.95 -1.5)
		(end 0.95 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "28358637-152c-449b-856c-d11866fc8838")
	)
	(fp_line
		(start 0.95 1.5)
		(end -0.95 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d57291fd-5450-436a-8418-049a87299516")
	)
	(fp_line
		(start -0.5 -1)
		(end -0.5 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "383e5bcf-b6f5-452f-a1b9-4a3a897bb83a")
	)
	(fp_line
		(start -0.5 1.25)
		(end 0.5 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "276c7f24-755a-4dc5-ac05-91459385629a")
	)
	(fp_line
		(start -0.25 -1.25)
		(end -0.5 -1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3b1fde62-6262-4456-ba24-8667a26a5c8a")
	)
	(fp_line
		(start 0.5 -1.25)
		(end -0.25 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3ae319a5-9baf-4068-9b88-b31537f45f6e")
	)
	(fp_line
		(start 0.5 -1.25)
		(end 0.5 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "99cd35a2-49ea-4238-be22-d0489203728c")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "ea4e1ecf-d2d2-415b-a681-d818605051be")
		(effects
			(font
				(size 0.55 0.55)
				(thickness 0.1)
			)
		)
	)
	(pad "1" smd rect
		(at -0.3875 -1 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "878ab5cf-ea29-4918-a6ed-5f204c199fec")
	)
	(pad "2" smd rect
		(at -0.3875 -0.5 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "9be2a8a3-c633-47aa-ae9b-87038e40bf00")
	)
	(pad "3" smd rect
		(at -0.35 0 270)
		(size 0.4 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "59e686c2-b782-403e-ab45-6c45344db88e")
	)
	(pad "4" smd rect
		(at -0.3875 0.5 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "53e3287f-4089-42bd-8529-26fbb8190ff1")
	)
	(pad "5" smd rect
		(at -0.3875 1 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "941b4bc3-583b-4771-87c9-31bae2f0ad6a")
	)
	(pad "6" smd rect
		(at 0.3875 1 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "14a169b8-fcc3-4a43-81fb-831039147c51")
	)
	(pad "7" smd rect
		(at 0.3875 0.5 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "cf2dcad5-ead3-4a0c-816f-14f19c0ea82c")
	)
	(pad "8" smd rect
		(at 0.4125 0 270)
		(size 0.4 0.575)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "0e5e283c-36b0-41bd-9e77-5b925f660b18")
	)
	(pad "9" smd rect
		(at 0.3875 -0.5 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "c1cfc78a-8163-45a4-93b9-363c8227b614")
	)
	(pad "10" smd rect
		(at 0.3875 -1 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections no)
		)
		(uuid "a2542167-d7e0-4a9d-90f7-8c165fcba4ad")
	)
	(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Diodes_UDFN-10_1.0x2.5mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)